Data/hora: 01/06/2024 03:11:30

Provedor de dados: 	5	
País: 	France	
Título: 	Protection par voie électrochimique de hublots immergés en milieu marin vis-à-vis des biosalissures

Electrochemical protection of windows immersed in seawater against biofouling	
Autores: 	Cachet, H.; Festy, Dominique; Folcher, G.; Mazeas, Florence; Tribollet, B.	
Data: 	2002	
Ano: 	2002	
Resumo: 	Biofouling reduction is a major problem for underwater instrumentation, involving optical measurements or viewing. This paper presents an effective window protection technique based on seawater electrolysis for producing active chlorine species. This is achieved by depositing a transparent conductive tin dioxide coating by spray pyrolysis. A number of laboratory and in situ experiments were performed in order to assess the effectiveness of this window protection technique. It was found that Sb doping was more efficient with respect to electrical energy management and long term SnO2 coating stability than the fluorine doping. In the present state of the art, biofouling prevention was proved to be effective over 5 months at least	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	https://archimer.ifremer.fr/doc/00480/59144/61772.pdf

DOI:10.1051/mattech/200290070037

https://archimer.ifremer.fr/doc/00480/59144/	
Editor: 	EDP Sciences	
Formato: 	application/pdf	
Fonte: 	Matériaux &amp; Techniques (0032-6895) (EDP Sciences), 2002 , Vol. 90 , N. 7-8 , P. 37-42	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use