Data/hora: 02/06/2024 16:02:17

Provedor de dados: | 5
País: | France
Título: | One-Single Extraction Procedure for the Simultaneous Determination of a Wide Range of Polar and Nonpolar Organic Contaminants in Seawater
Autores: | Fauvelle, Vincent; Castro-jimenez, Javier; Schmidt, Natascha; Carlez, Benoit; Panagiotopoulos, Christos; Sempere, Richard.
Data: | 2018-08
Ano: | 2018
Palavras-chave: | Plastic additive; Seawater; Organic contaminants; Legacy contaminants; Phtalates; Bisphenol; Organophosphate esters.
Resumo: | A rapid analytical method including one-single solid-phase extraction (SPE) procedure followed by gas and liquid chromatography coupled with high resolution mass spectrometry detection (GC-MS and LC-HRMS respectively) was developed for the quantification of 40 organic compounds (1.6 &lt; log K-ow &lt; 9.5) in seawater including both legacy and emerging contaminants, with a focus on the most common plastic organic additives. This new method allowed for the analyses of nine organophosphate esters (OPEs), seven phthalates (PAEs), six bisphenols (BPs), five perfluorinated compounds (PFCs), and thirteen legacy organochlorinated compounds (OCs, including polychlorobiphenyles and pesticides) with recoveries in the ranges of 57-124% for OPEs, 52-163% for PAEs, 64-118% for BPs, 63-124% for PFCs, and 40-95% for OCs. As a result of (i) strict cleanup protocols, (ii) material, and solvent selection, and (iii) the use of an ISO 6 cleanroom for sample treatment, the procedural blank levels were always lower than 5 ng L-1, even for the most abundant and ubiquitous compounds like tris-(2-chloro, 1-methylethyl) phosphate (TCPP) and diethylhexyl phthalate (DEHP). The quantification limits were in the ranges of 0.03-0.75 ng L-1 for OPEs, 0.03-0.25 ng L-1 for PAEs, 0.1-5 ng L-1 for BPs, 0.1-8 ng L-1 for PFCs, and 0.02-1.1 ng L-1 for OCs, matching seawater analysis requirements. Dissolved water phase samples collected in Marseille Bay (NW Mediterranean Sea) were analyzed using the developed method reveling the concentration of PAEs up to 140 ng L-1 (DEHP) and that of OCs up to 70 ng L-1 (ot-endosulfan). For the first time, we also provided the concentrations of OPEs (TCPP up to 450 ng L-1), BPs (bisphenol Sup to 123 ng L-1), and PFCs (PFOS up to 5 ng L-1) in this area. A sampling station close to the municipal waste water treatment plant outfall exhibited the highest concentration levels for all compounds.
Tipo: | Text
Idioma: | Inglês

Identificador:

https://archimer.ifremer.fr/doc/00645/75716/76697.pdf

https://archimer.ifremer.fr/doc/00645/75716/76698.docx

DOI:10.3389/fmars.2018.00295

https://archimer.ifremer.fr/doc/00645/75716/

Editor: | Frontiers Media Sa
Formato: | application/pdf
Fonte: | Frontiers In Marine Science (2296-7745) (Frontiers Media Sa), 2018-08 , Vol. 5 , N. 295 , P. 10p.

Fonte:

info:eu-repo/semantics/openAccess

restricted use