Data/hora: 01/06/2024 09:28:11

Provedor de dados: | 5
País: | France
Título: | Modélisation hydrodynamique de la dispersion à court terme dans une mer macrotidale: validation par des mesures à haute résolution de radiotraceurs solubles
Autores: | Bailly Du Bois, Pascal; Dumas, Franck.
Data: | 2004-09
Ano: | 2004
Palavras-chave: | Validation; Tritium; Dispersion; North sea; Hydrodynamic model; Validation; Tritium; Dispersion; Manche; Modèle.
Resumo: | DISPRO project aims to validate hydrodynamic models dispersion parameters by field data for the short-term (hours to week) and short distances (100 meters to 30 km). This project is based on a 2D instantaneous currents model with a mesh size of 110 m, coupled with high frequency field data collected in the release plume. At this step of the works, measurements confirm the reliability of the model during six hours following a release. This validation made possible developpement of models with known incertitude to simulate dispersion of dissolved substances in realistic conditions for normal or accidental situations in macrotidal seas.
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/2004/acte-564.pdf
Editor: | VIIIèmes Journées Nationales Génie Civil ¿ Génie Côtier, Compiègne, 7-9 septembre 2004
Relação: | http://archimer.ifremer.fr/doc/00000/564/
Formato: | application/pdf