Data/hora: 07/06/2024 05:47:44

Provedor de dados: 	5	
País: 	France	
Título: 	Modeling of tidally-induced hydro-sedimentary processes in the coastal zone of the southern part of the dover strait	
Autores: 	Chapalain, G; Smaoui, H; Lepretre, A; Nguyen, Kd; Ouahsine, A; Tessier, B.	
Data: 	1993	
Ano: 	1993	
Palavras-chave: 	DOVER STRAIT; TIDAL CURRENTS; COASTAL SEDIMENTS; HYDRO-SEDIMENTARY PROCESSES; MODELING.	
Resumo: 	The present paper deals with the modelling of hydro-sedimentary processes in the coastal area near Cape Gris-Nez and Cape Blanc-Nez (Dover Strait). The modelling procedure consists in coupling different hydro-sedimentary process models with a high spatial resolution two-dimensional tidal flow model (Nguyen and Ouahsine, 1992). The sediment transport models used include two semi-empirical models based on a dimensionless analysis and energetic concepts (Ackers and White, 1973; Engelund and Hansen, 1967), and a more heuristic cu (concentration times velocity) model (van Rijn, 1984 a; b). All these models are applied to predict instantaneous and tidally-integrated sediment transports in the area under investigation.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00100/21140/18760.pdf	
Editor: 	Gauthier-Villars	
Relação: 	http://archimer.ifremer.fr/doc/00100/21140/	
Formato: 	application/pdf	
Fonte: 	Oceanologica Acta (0399-1784) (Gauthier-Villars), 1993 , Vol. 16 , N. 5-6 , P. 517-529