Data/hora: 01/06/2024 06:23:48

Provedor de dados: 	5	
País: 	France	
Título: 	CATARINA 2012-Leg 1 - CTD-O2 Data report	
Autores: 	Branellec, Pierre; Lherminier, Pascale; Desprez De Gesincourt, Floriane.	
Data: 	2013-12	
Ano: 	2013	
Resumo: 	The CATARINA Leg1 cruise was carried out from June 22 to July 24 2012 on board the B/O Sarmiento de Gamboa, under the scientific supervision of Aida Rios (CSIC-IIM). It included the occurrence of the OVIDE hydrological section that was performed in June 2002, 2004, 2006, 2008 and 2010, as part of the CLIVAR program (name A25) ), and under the supervision of Herlé Mercier (CNRSLPO). This section begins near Lisbon (Portugal), runs through the West European Basin and the Iceland Basin, crosses the Reykjanes Ridge (300 miles north of Charlie-Gibbs Fracture Zone, and ends at Cape Hoppe (southeast tip of Greenland). The objective of this repeated hydrological section is to monitor the variability of water mass properties and main current transports in the basin, complementing the international observation array relevant for climate studies. In addition, the Labrador Sea was partly sampled (stations 101-108) between Greenland and Newfoundland, but heavy weather conditions prevented the achievement of the section south of 53°40’N. The quality of CTD data is essential to reach the first objective of the CATARINA project, i.e. to quantify the Meridional Overturning Circulation and water mass ventilation changes and their effect on the changes in the anthropogenic carbon ocean uptake and storage capacity. The CATARINA project was mainly funded by the Spanish Ministry of Sciences and Innovation and co-funded by the Fondo Europeo de Desarrollo Regional.  The hydrological OVIDE section includes 95 surface-bottom stations from coast to coast, collecting profiles of temperature, salinity, oxygen and currents, spaced by 2 to 25 Nm depending on the steepness of the topography. The position of the stations closely follows that of OVIDE 2002. In addition, 8 stations were carried out in the Labrador Sea. From the 24 bottles closed at various depth at each stations, samples of sea water are used for salinity and oxygen calibration, and for measurements of biogeochemical components that are not reported here. The data were acquired with a Seabird CTD (SBE911+) and an SBE43 for the dissolved oxygen, belonging to the Spanish UTM group. The software SBE data processing was used after decoding and cleaning the raw data. Then, the LPO matlab toolbox was used to calibrate and bin the data as it was done for the previous OVIDE cruises, using on the one hand pre and post-cruise calibration results for the pressure and temperature sensors (done at Ifremer) and on the other hand the water samples of the 24 bottles of the rosette at each station for the salinity and dissolved oxygen data. A final accuracy of 0.002°C, 0.002 psu and 0.04 ml/l (2.3 umol/kg) was obtained on final profiles of temperature, salinity and dissolved oxygen, compatible with international requirements issued from the WOCE program.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00353/46406/46280.pdf

http://archimer.ifremer.fr/doc/00353/46406/	
Formato: 	application/pdf	
Fonte: 	2013 Ifremer

info:eu-repo/semantics/openAccess

restricted use