Data/hora: 07/06/2024 03:32:32

Provedor de dados: 	5	
País: 	France	
Título: 	Rejets urbains. Volet Manche - Atlantique - Site de Morlaix - Etudes sédimentologique et Bathymétrique de l' estuaire de Morlaix	
Autores: 	Bassoullet, Philippe; L'Yavanc, Jacky; Guillaud, Jean-francois; Loarer, Ronan; Breton, Marguerite.	
Data: 	1987-09	
Ano: 	1987	
Palavras-chave: 	Rejet urbain; Sédiment; Granulométrie; Hydrodynamique; Modèle de transport particulaire; Sable; Vase; Estuaire de Morlaix.; Urban wastes; Model; Sediment; Granulometry; Hydrodynamics; Sand; Mud; Sedimentary transport model; Morlaix estuary.	
Resumo: 	In order to increase our knowledge about sediment transport in the bay and maritime part of the River of Morlaix (Finistère), measurernènts have been perforrned on site. This report gives the granulometrical and physical parameters of the sediments as weIl as the hydrodynamics, used for a model of particulate transport in the area. The rnodel and its application will be published later	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/00345/45658/45293.pdf

http://archimer.ifremer.fr/doc/00345/45658/	
Formato: 	application/pdf	
Fonte: 	1987 Ifremer

info:eu-repo/semantics/openAccess

restricted use