Data/hora: 05/06/2024 03:12:50

Provedor de dados: | 5
País: | France
Título: | A dissolved oxygen calibration bench
Autores: | Salvetat, Florence; Lamandé, Nolwenn; Le Bihan, Caroline; Compère, Chantal.
Data: | 2013
Ano: | 2013
Resumo: | This paper presents a metrology bench dedicated to the calibration of optical dissolved oxygen sensors. This set up is used at Ifremer metrology laboratory to calibrate dissolved oxygen sensors integrated on oceanographic probes. The characterization of the bench is seen through the analysis of its stability and its homogeneity. An application is proposed on the calibration of Aanderaa 3835 and 4330 optodes.
Tipo: | Text
Idioma: | Inglês

Identificador:

https://archimer.ifremer.fr/doc/00479/59094/61732.pdf

DOI:10.1051/metrology/201310003

https://archimer.ifremer.fr/doc/00479/59094/

Editor: | 16th International Congress of Metrology (EDP Sciences). 1003, 5p.
Formato: | application/pdf

Fonte:

info:eu-repo/semantics/openAccess

restricted use