Data/hora: 06/06/2024 08:53:29

Provedor de dados: | 5
País: | France
Título: | Metal measurement in aquatic environments by passive sampling methods: Lessons learning from an in situ intercomparison exercise
Autores: | Dabrin, A.; Ghestem, J. -p.; Uher, E.; Gonzalez, Jean-louis; Allan, I. J.; Schintu, M.; Montero, N.; Balaam, J.; Peinerud, E.; Miege, C.; Coquery, M.
Data: | 2016-01
Ano: | 2016
Palavras-chave: | DGT; Uncertainty; Blank; Continental waters; Coastal waters.
Resumo: | Passive sampling devices (PS) are widely used for pollutant monitoring in water, but estimation of measurement uncertainties by PS has seldom been undertaken. The aim of this work was to identify key parameters governing PS measurements of metals and their dispersion. We report the results of an in situ intercomparison exercise on diffusive gradient in thin films (DGT) in surface waters. Interlaboratory uncertainties of time-weighted average (TWA) concentrations were satisfactory (from 28% to 112%) given the number of participating laboratories (10) and ultra-trace metal concentrations involved. Data dispersion of TWA concentrations was mainly explained by uncertainties generated during DGT handling and analytical procedure steps. We highlight that DGT handling is critical for metals such as Cd, Cr and Zn, implying that DGT assembly/dismantling should be performed in very clean conditions. Using a unique dataset, we demonstrated that DGT markedly lowered the LOQ in comparison to spot sampling and stressed the need for accurate data calculation.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00294/40560/39614.pdf

DOI:10.1016/j.envpol.2015.08.049

http://archimer.ifremer.fr/doc/00294/40560/

Editor: | Elsevier Sci Ltd
Formato: | application/pdf
Fonte: | Environmental Pollution (0269-7491) (Elsevier Sci Ltd), 2016-01 , Vol. 208 , P. 299-308

Fonte:

2015 Elsevier Ltd. All rights reserved.

info:eu-repo/semantics/openAccess

restricted use