Data/hora: 13/06/2024 05:00:43

Provedor de dados: | 5
País: | France
Título: | Observation of tropical cyclones by high-resolution scatterometry
Autores: | Quilfen, Yves; Chapron, Bertrand; Elfouhaily, Tanos; Katsaros, Kristina; Tournadre, Jean.
Data: | 1998-04-15
Ano: | 1998
Resumo: | Unprecedented views of surface wind fields in tropical cyclones thereafter TCs) are provided by the European Remote Sensing Satellite (ERS) C band scatterometer. Scatterometer measurements at C band are able to penetrate convective storms clouds, observing the surface wind fields with good accuracy. However the resolution of the measurements (50x50 km(2)) limits the interpretation of the scatterometer signals in such mesoscale events. The strong gradients of the surface wind existing at scales of a few kms are smoothed in the measured features such as the intensity and location of the wind maxima, and the position of the center. Beyond the ERS systems, the scatterometers on-board the ADEOS and METOP satellites, designed by the Jet Propulsion Laboratory and by the European Space Agency, respectively, will be able to produce measurements of the backscattering coefficient at about 25x25 km(2) resolution. A few sets of ERS-1 orbits sampling TC events were produced with an experimental 25x25 km(2) resolution. Enhancing the resolution by a factor of 2 allows location of the wind maxima and minima in a TC with a much better accuracy than at 50 km resolution. In addition, a better resolution reduces the geophysical noise (variability of wind speed within the cell and effect of rain) that dominates the radiometric noise and hence improves the definition of the backscattering measurements. A comprehensive analysis of the backscattering measurements in the case of high winds and high sea states obtained within TCs is proposed in order to refine the interpretation of the wind vector derived from a backscattering model that is currently only calibrated up to moderate winds (&lt; 20 m/s) in neutral conditions. Observations of the TOPEX-POSEIDON dual-frequency altimeter are also used for that purpose. Patterns of the surface winds in TCs are described and characteristic features concerning asymmetries in the maximum winds and in the divergence field are discussed.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00251/36257/34805.pdf

DOI:10.1029/97JC01911

http://archimer.ifremer.fr/doc/00251/36257/

Editor: | American Geophysical Union
Formato: | application/pdf
Fonte: | Journal of Geophysical Research ( JGR ) - Oceans (0148-0227) (American Geophysical Union), 1998-04-15 , Vol. 103 , N. C4 , P. 7767-7786

Fonte:

Copyright 1998 by the American Geophysical Union.

info:eu-repo/semantics/openAccess

restricted use