Data/hora: 06/06/2024 00:47:31

Provedor de dados: | 5
País: | France
Título: | Advances in measuring ocean salinity with an optical sensor
Autores: | Le Menn, Marc; De La Tocnaye, J. L. De Bougrenet; Grosso, P.; Delauney, Laurent; Podeur, Christian; Brault, P.; Guillerme, O.
Data: | 2011-11
Ano: | 2011
Palavras-chave: | Refractive index; Seawater; Density; Salinity; Refractometer.
Resumo: | Absolute salinity measurement of seawater has become a key issue in thermodynamic models of the oceans. One of the most direct ways is to measure the seawater refractive index which is related to density and can therefore be related to the absolute salinity. Recent advances in high resolution position sensitive devices enable us to take advantage of small beam deviation measurements using refractometers. This paper assesses the advantages of such technology with respect to the current state-of-the-art technology. In particular, we present the resolution dependence on refractive index variations and derive the limits of such a solution for designing seawater sensors well suited for coastal and deep-sea applications. Particular attention has been paid to investigate the impact of environmental parameters, such as temperature and pressure, on an optical sensor, and ways to mitigate or compensate them have been suggested here. The sensor has been successfully tested in a pressure tank and in open oceans 2000 m deep.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00052/16295/13899.pdf

DOI:10.1088/0957-0233/22/11/115202

Editor: | Iop Publishing Ltd
Relação: | http://archimer.ifremer.fr/doc/00052/16295/
Formato: | application/pdf
Fonte: | Measurement Science &amp; Technology (0957-0233) (Iop Publishing Ltd), 2011-11 , Vol. 22 , N. 11 , P. 1-8
Fonte: | 2011 IOP Publishing Ltd