Data/hora: 01/06/2024 09:27:35

Provedor de dados: | 5
País: | France
Título: | MAREL Carnot data and metadata from Coriolis Data Centre
Autores: | Lefebvre, Alain.
Data: | 2015-11
Ano: | 2015
Palavras-chave: | MAREL Carnot; Buoy; Observing system; High frequency; Eastern English Channel; Estimated sea level; Gust wind speed; Wind from direction relative true north; Horizontal wind speed; Relative humidity; Light irradiance surface PAR; Sea temperature; Practical salinity; Ph; Dissolved oxygen; Fluorescence; Turbidity; Nitrate + nitrite; Phosphate; Silicate.
Resumo: | The MAREL (Mesures Automatisées en Réseau pour l’Environnement Littoral) Carnot system developed and implemented by Ifremer (French Research Institute for Exploitation of the sea) in 2004 is a moored buoy equipped with physico-chemical and biological measuring devices working in continuous and autonomous conditions. The system is located in the Boulogne-sur-Mer harbor (eastern English Channel) influenced both by marine coastal and fresh waters. The measuring station is equipped with high performance systems for seawater analysis and near real time data transmission. These system record with a high frequency resolution (20 minutes), the following parameters: estimated sea level, gust wind speed, wind from direction relative true north, horizontal wind speed, relative humidity, light irradiance surface PAR, sea temperature, practical salinity, ph, dissolved oxygen, fluorescence, turbidity. For nitrate + nitrite, phosphate, silicate parameters the sampling frequency is set to 12 hours.
Tipo: | Dataset

Identificador:

DOI:10.17882/39754

http://dx.doi.org/10.17882/39754

Editor: | Seanoe
Fonte: | restricted use