Data/hora: 06/06/2024 08:43:12

Provedor de dados: 	5	
País: 	France	
Título: 	Ambient flow velocity and resulting clearance rates of the terebellid polychaete Lanice conchilega (Pallas, 1766)	
Autores: 	Denis, L; Desroy, Nicolas; Ropert, Michel.	
Data: 	2007-10	
Ano: 	2007	
Palavras-chave: 	Recirculating flume; Feeding activity; Terebellidea; Polychaetes; Clearance rate; Lanice conchilega.	
Resumo: 	A laboratory flume study was conducted to determine the effect of flow velocity on clearance rates of the Polychaeta Terebellidea Lanice conchilega (Pallas, 1966). Using sets of 75 individuals collected along the east coast of the English Channel, we measured clearance rates at five flow velocities of approximate to 4, 9, 15, 22 and 27 cm s(-1) with a culture of the diatom Chaetoceros calcitrans as food source. During each control (without polychaetes) or clearance (with Lanice conchilega) experiment, in vivo fluorescence was continuously monitored. Further HPLC analysis confirmed the sediment resuspension for the highest flow velocities tested, indicating the need for 'corrections' from control experiments. The global pattern resulted in a dome-shaped curve, with a corrected clearance rate per individual increasing with flow velocity from an average value of 0.091 +/- 0.041 L h(-1) gDW(-1) at 4 cm s(-1) up to a maximal value of0.171 +/- 0.046 L h(-1) ind(-1) at 15 cm s(-1) and decreasing for higher flow velocity (0.063 +/- 0.029 L h(-1) ind(-1) at 27 cm s(-1)). When non-nalised to average Dry Weight (DW), the clearance rates varied in a wider range, with maximal clearance rates of up to 0.749 L h(-1) gDW(-1) and a marked dome-shaped structure for small individuals (11.9 +/- 5.4 mg Ash Free Dry Weight), whereas larger individuals (up to 30 mg AFDW) showed maximal clearance rates of around 0.400 L h(-1) gDW(-1). Our results indicate the need to take flow velocity into account in estimating the ecological impact of filter-feeding polychactes on available food, as large budget underestimates may arise from clearance rates measured in non-controlled flow velocity. (C) 2007 Elsevier B.V. All rights reserved.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/2007/publication-3418.pdf

DOI:10.1016/j.seares.2007.03.005	
Editor: 	Elsevier	
Relação: 	http://archimer.ifremer.fr/doc/00000/3418/	
Formato: 	application/pdf	
Fonte: 	Journal of Sea Research (1385-1101) (Elsevier), 2007-10 , Vol. 58 , N. 3 , P. 209-219	
Fonte: 	2007 Elsevier B.V. All rights reserved