Data/hora: 14/06/2024 12:51:43

Provedor de dados: 	5	
País: 	France	
Título: 	Cinétique d'épuration in-situ de moules contaminés par un gas-oil	
Autores: 	Michel, Pierre.	
Data: 	1976-06	
Ano: 	1976	
Resumo: 	On November 17th 1975, the tanker "Port de Bouc" with 1 700 t. of fuel n° 2 on board run aground in Saint-Brieuc Bight and 470 t. of this product escaped. The mussel farming zones situated between 10 and 20 km from the oil spill place were rapidly polluted within a few days. The appraised mussels value was 2 millions US dollars. A regular survey of the situation was made and 52 samples were analysed. After 3 days, the maximum of contamination was measured in a sample (505 mg/kg of wet flesh against 16 mg/kg in a non polluted check sample) the maximum pollution for the whole bight was measured after 15 days (the average was 220 mg/kg). First, the release was fast during 1 month and characterized by the total elimination of n-paraffins. Nevertheless, the petroleum taste remained during more than 3 months. Five months were necessary for a complete removal. No mortality was observed and mussels had a normal growing rate during this period.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/1976/publication-7121.pdf	
Editor: 	ISTPM	
Relação: 	http://archimer.ifremer.fr/doc/00000/7121/	
Formato: 	application/pdf	
Fonte: 	Science et Pêche (0036-8350) (ISTPM), 1976-06 , Vol. 259 , P. 1-7	
Fonte: 	Ifremer