Data/hora: 05/06/2024 06:24:30

Provedor de dados: 	5	
País: 	France	
Título: 	Experimental study of the turbulence intensity effects on marine current turbines behaviour. Part I: One single turbine	
Autores: 	Mycek, Paul; Gaurier, Benoit; Germain, Gregory; Pinon, Gregory; Rivoalen, Elie.	
Data: 	2014-06	
Ano: 	2014	
Palavras-chave: 	Marine current turbine; Performance; Wake; Turbulence; Experiment; Flume tank.	
Resumo: 	The ambient turbulence intensity in the upstream flow plays a decisive role in the behaviour of horizontal axis marine current turbines.  Experimental trials, run in the IFREMER flume tank in Boulogne-Sur-Mer (France) for two different turbulence intensity rates, namely 3% and 15%, are presented. They show, for the studied turbine configuration, that while the wake of the turbine is deeply influenced by the ambient turbulence conditions, its mean performances turn out to be slightly modified.  The presented conclusions are crucial in the view of implanting second generation turbines arrays. In addition, complete and detailed data sets (wake profiles and performance graphs) are made available to the scientific community in order to encourage further comparisons.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00175/28647/27171.pdf

DOI:10.1016/j.renene.2013.12.036	
Editor: 	Pergamon-elsevier Science Ltd	
Relação: 	http://archimer.ifremer.fr/doc/00175/28647/	
Formato: 	application/pdf	
Fonte: 	Renewable Energy (0960-1481) (Pergamon-elsevier Science Ltd), 2014-06 , Vol. 66 , P. 729-746	
Fonte: 	2014 Elsevier Ltd. All rights reserved.