Data/hora: 01/06/2024 09:20:45

Provedor de dados: 	5	
País: 	France	
Título: 	Optical algorithms at satellite wavelengths for Total Suspended Matter in tropical coastal waters	
Autores: 	Ouillon, Sylvain; Douillet, Pascal; Petrenko, Anne; Neveux, Jacques; Dupouy, Cecile; Froidefond, Jean-marie; Andrefouet, Serge; Munoz-caravaca, Alain.	
Data: 	2008-07	
Ano: 	2008	
Palavras-chave: 	Ocean color; Remote sensing; Sediment transport; Suspended matter; Turbidity; New Caledonia; Cuba; Fiji.	
Resumo: 	Is it possible to derive accurately Total Suspended Matter concentration or its proxy, turbidity, from remote sensing data in tropical coastal lagoon waters? To investigate this question, hyperspectral remote sensing reflectance, turbidity and chlorophyll pigment concentration were measured in three coral reef lagoons. The three sites enabled us to get data over very diverse environments: oligotrophic and sediment-poor waters in the southwest lagoon of New Caledonia, eutrophic waters in the Cienfuegos Bay (Cuba), and sediment-rich waters in the Laucala Bay (Fiji). In this paper, optical algorithms for turbidity are presented per site based on 113 stations in New Caledonia, 24 stations in Cuba and 56 stations in Fiji. Empirical algorithms are tested at satellite wavebands useful to coastal applications. Global algorithms are also derived for the merged data set (193 stations). The performances of global and local regression algorithms are compared. The best one-band algorithms on all the measurements are obtained at 681 nm using either a polynomial or a power model. The best two-band algorithms are obtained with R412/R620, R443/R670 and R510/R681. Two three-band algorithms based on Rrs620. Rrs681/Rrs412 and Rrs620. Rrs681/Rrs510 also give fair regression statistics. Finally, we propose a global algorithm based on one or three bands: turbidity is first calculated from Rrs681 and then, if &lt; 1 FTU, it is recalculated using an algorithm based on Rrs620. Rrs681/Rrs412. On our data set, this algorithm is suitable for the 0.2-25 FTU turbidity range and for the three sites sampled (mean bias: 3.6 %, rms: 35%, mean quadratic error: 1.4 FTU). This shows that defining global empirical turbidity algorithms in tropical coastal waters is at reach.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	https://archimer.ifremer.fr/doc/00203/31417/29808.pdf

DOI:10.3390/s8074165

https://archimer.ifremer.fr/doc/00203/31417/	
Editor: 	Molecular Diversity Preservation Int	
Formato: 	application/pdf	
Fonte: 	Sensors (1424-8220) (Molecular Diversity Preservation Int), 2008-07 , Vol. 8 , N. 7 , P. 4165-4185	
Fonte: 	2008 by the authors; licensee Molecular Diversity Preservation International, Basel, Switzerland. This article is an open-access article distributed under the terms and conditions of the Creative Commons Attribution license (http://creativecommons.org/licenses/by/3.0/).

info:eu-repo/semantics/openAccess

restricted use