Data/hora: 07/06/2024 03:01:13

Provedor de dados: 	5	
País: 	France	
Título: 	Développement et essais d’un salinomètre optique pour l’océanographie

Development of an optical salinometer for oceanography	
Autores: 	Le Menn, Monique; Malardé, Damien; David, Arnaud; Brault, Patrice; Grosso, Philippe; De Bougrenet De La Tocnaye, Jean-louis; Le Reste, Serge; Podeur, Christian.	
Data: 	2016-06	
Ano: 	2016	
Palavras-chave: 	Salinity; Density; Ocean; Seawater; Refractive index; Sensor.	
Resumo: 	Salinity is the essential parameter for ocean dynamics studies. Its definition and using in the equations used to calculate the thermodynamic properties of seawater, were revised in 2010, opening the possibility of new sensors developments. In this context, NOSS (NKE Optical Salinity Sensor) has emerged as one of the first underwater instrument for in situ refractive index measurement in the past years open up the scope of possibilities to access to density parameter. This achievement is the fruit of the cooperation between several institutions and the fruit of several years of developments and trials. NOSS sensor is designed to be deployed in coastal environment and open-ocean waters up to 2000m, especially on profiling floats of the Argo network.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	https://archimer.ifremer.fr/doc/00664/77601/79616.pdf

DOI:10.3166/I2M.15.1-2.53-63

https://archimer.ifremer.fr/doc/00664/77601/	
Editor: 	International Information and Engineering Technology Association	
Formato: 	application/pdf	
Fonte: 	Instrumentation Mesure Métrologie (1631-4670) (International Information and Engineering Technology Association), 2016-06 , Vol. 15 , N. 1-2 , P. 53-63	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use