Data/hora: 15/06/2024 06:55:05

Provedor de dados: 	5	
País: 	France	
Título: 	Monitoring Marine Habitats With Photogrammetry: A Cost-Effective, Accurate, Precise and High-Resolution Reconstruction Method	
Autores: 	Marre, Guilhem; Holon, Florian; Luque, Sandra; Boissery, Pierre; Deter, Julie.	
Data: 	2019-05	
Ano: 	2019	
Palavras-chave: 	Underwater photogrammetry; Resolution; Accuracy; Precision; 3D habitat mapping; Marine ecology.	
Resumo: 	Underwater photogrammetry has been increasingly used to study and monitor the three-dimensional characteristics of marine habitats, despite a lack of knowledge on the quality and reliability of the reconstructions. More particularly, little attention has been paid to exploring and estimating the relative contribution of multiple acquisition parameters on the model resolution (distance between neighbor vertices), accuracy (closeness to true positions/measures) and precision (variability of positions/measures). On the other hand, some studies used expensive or cumbersome camera systems that can restrict the number of users of this technology for the monitoring of marine habitats. This study aimed at developing a simple and cost-effective protocol able to produce accurate and reproducible high-resolution models. Precisely, the effect of the camera system, flying elevation, camera orientation and number of images on the resolution and accuracy of marine habitat reconstructions was tested through two experiments. A first experiment allowed for testing all combinations of acquisition parameters through the building of 192 models of the same 36 m(2) study site. The flying elevation and camera system strongly affected the model resolution, while the photo density mostly affected bundle adjustment accuracy and total processing time. The camera orientation, in turn, mostly affected the reprojection error. The best combination of parameters was used in a second experiment to assess the accuracy and precision of the resulting reconstructions. The average model resolution was 3.4 mm, and despite a decreasing precision in the positioning of markers with distance to the model center (0.33, 0.27, and 1.2 mm/m Standard Deviation (SD) in X, Y, Z, respectively), the measures were very accurate and precise: 0.08% error +/- 0.06 SD for bar lengths, 0.36% +/- 0.51 SD for a rock model area and 0.92% +/- 0.54 SD for its volume. The 3D geometry of the rock only differed by 1.2 mm +/- 0.8 SD from the ultra-high resolution in-air reference. These results suggest that this simple and cost-effective protocol produces accurate and reproducible models that are suitable for the study and monitoring of marine habitats at a small reef scale.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	https://archimer.ifremer.fr/doc/00501/61272/64848.pdf

DOI:10.3389/fmars.2019.00276

https://archimer.ifremer.fr/doc/00501/61272/	
Editor: 	Frontiers Media Sa	
Formato: 	application/pdf	
Fonte: 	Frontiers In Marine Science (2296-7745) (Frontiers Media Sa), 2019-05 , Vol. 6 , N. 276 , P. 15p.	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use