Data/hora: 05/06/2024 02:27:11

Provedor de dados: 	52	
País: 	Brazil	
Título: 	Azo Dye Mineralization by Phanerochaete Chysosporium in a Sequencing Bath Reactor	
Autores: 	Wanderley,Carlos Ronald Pessoa; Andrade,Marcus Vinícius; Pereira,Luciana José; Silva,Gloria Maria Marinho; Pessoa,Kelly Rodrigues.	
Data: 	2018-01-01	
Ano: 	2018	
Palavras-chave: 	Biodegradation; Congo red; Phanerochaete chrysosporium; Sequential bioreactors.	
Resumo: 	ABSTRACT The mineralization of the azo dye congo red by the fungi Phanerochaete chrysosporium was studied in two sequential batch bioreactors (R1 and R2), operated in cycles of 48 h (step I) and 24 h (step II). In step I, glucose concentration was 1 g.L-1 in both reactors and in step II, 1 g.L-1 of glucose was maintained in R1, but R2 received no addition of glucose. In step I, the average dye removal efficiencies were 76 ± 29 % (R1) and 53 ± 15% (R2), while in step II the averages recorded for dye removal for R1 and R2 were 84 ± 15 and 70 ± 28%, respectively. The rates of dye removal were 0.04 h-1 in R1 and 0.03 h-1 in R2 in step I. Higher rates were obtained in step II, 0,07 h-1 and 0,02 h-1 for R1 and R2, respectively. The highest dye removal occurred in R1 and, in R2, the residual dye was further removed. Laccase was the oxidised at higher amount, in step I was 54 μmol.min-1 for R1 and 38 μmolmin-1 for R2. The proposed treatment system was very effective in removing the azo dye, however the mineralization may not be complete and some by-products may have been formed, according to spectrofotometric analysis, were the peak corresponding to benzene, 220 nm, persisted.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132018000100606	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/1678-4324-2018180195	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.61 2018	
Fonte: 	info:eu-repo/semantics/openAccess