Data/hora: 06/06/2024 01:40:00

Provedor de dados: | 52
País: | Brazil
Título: | Fed batch enzymatic saccharification of food waste improves the sugar concentration in the hydrolysates and eventually the ethanol fermentation by Saccharomyces cerevisiae H058
Autores: | Yan,Shoubao; Yao,Jianming; Yao,Liming; Zhi,Zhijun; Chen,Xiangsong; Wu,Jingyong.
Data: | 2012-04-01
Ano: | 2012
Palavras-chave: | Food waste; Enzymatic hydrolysis; Hydrolysates; Fermentation; Ethanol production.
Resumo: | The enzymatic hydrolysis of food waste by commercially available enzymes and the subsequent ethanol fermentation of the hydrolysates by Saccharomyces cerecisiae H058 were studied in this work. The optimum batch enzymatic conditions were found to be saccharification pH of 4.5, temperature of 55!, glucoamylase concentration of 120 u/g, α-amylase concentration of 10 u/g, solid-liquid ratio of 1: 0.75 (w/w). Fed batch hydrolysis process was started with a solid-liquid ratio of 1: 1 (w/w), with solid food waste added at time lapse of 2 h to get a final solid-liquid ratio of 1: 0.5 (w/w). After 4 h of reaction, the reducing sugar concentration reached 194.43 g/L with a enzymatic digestibility of 93.12%. Further fermentation of the batch and fed batch enzymatic hydrolysates, which contained reducing sugar concentration of 131.41 and 194.43 g/L respectively, was performed using Saccharomyces cerevisiae H058, 62.93 and 90.72 g/L ethanol was obtained within 48 h.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132012000200002
Editor: | Instituto de Tecnologia do Paraná - Tecpar
Relação: | 10.1590/S1516-89132012000200002
Formato: | text/html
Fonte: | Brazilian Archives of Biology and Technology  v.55 n.2 2012
Fonte: | info:eu-repo/semantics/openAccess