Data/hora: 08/06/2024 10:55:41

Provedor de dados: | 58
País: | Brazil
Título: | Bioleaching of gold, copper and nickel from waste cellular phone PCBs and computer goldfinger motherboards by two Aspergillus nigerstrains
Autores: | Madrigal-Arias,Jorge Enrique; Argumedo-Delira,Rosalba; Alarcón,Alejandro; Mendoza-López,Ma. Remedios; García-Barradas,Oscar; Cruz-Sánchez,Jesús Samuel; Ferrera-Cerrato,Ronald; Jiménez-Fernández,Maribel.
Data: | 2015-09-01
Ano: | 2015
Palavras-chave: | Bioleaching; PCBs; Aspergillus; Gold; WEEE.
Resumo: | In an effort to develop alternate techniques to recover metals from waste electrical and electronic equipment (WEEE), this research evaluated the bioleaching efficiency of gold (Au), copper (Cu) and nickel (Ni) by two strains of Aspergillus niger in the presence of gold-plated finger integrated circuits found in computer motherboards (GFICMs) and cellular phone printed circuit boards (PCBs). These three metals were analyzed for their commercial value and their diverse applications in the industry. Au-bioleaching ranged from 42 to 1% for Aspergillus niger strain MXPE6; with the combination of Aspergillus niger MXPE6 + Aspergillus niger MX7, the Au-bioleaching was 87 and 28% for PCBs and GFICMs, respectively. In contrast, the bioleaching of Cu by Aspergillus niger MXPE6 was 24 and 5%; using the combination of both strains, the values were 0.2 and 29% for PCBs and GFICMs, respectively. Fungal Ni-leaching was only found for PCBs, but with no significant differences among treatments. Improvement of the metal recovery efficiency by means of fungal metabolism is also discussed.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822015000300707
Editor: | Sociedade Brasileira de Microbiologia
Relação: | 10.1590/S1517-838246320140256
Formato: | text/html
Fonte: | Brazilian Journal of Microbiology  v.46 n.3 2015
Fonte: | info:eu-repo/semantics/openAccess