Data/hora: 09/06/2024 10:36:12

Provedor de dados: 	63	
País: 	Brazil	
Título: 	Planosol soil sample size for computerized tomography measurement of physical parameters	
Autores: 	Pedrotti,Alceu; Pauletto,Eloy Antonio; Crestana,Silvio; Cruvinel,Paulo Estevão; Vaz,Carlos Manoel Pedro; Naime,João de Mendonça; Silva,Alvaro Macedo da.	
Data: 	2003-12-01	
Ano: 	2003	
Palavras-chave: 	Lowland; Albaqualf; Bulk density; Compaction; Soil moisture.	
Resumo: 	Computerized tomography (CT) is an important tool in Soil Science for noninvasive measurement of density and water content of soil samples. This work aims to describe the aspects of sample size adequacy for Planosol (Albaqualf) and to evaluate procedures for statistical analysis, using a CT scanner with a 241Am source. Density errors attributed to the equipment are 0.051 and 0.046 Mg m-3 for horizons A and B, respectively. The theoretical value for sample thickness for the Planosol, using this equipment, is 4.0 cm for the horizons A and B. The ideal thickness of samples is approximately 6.0 cm, being smaller for samples of the horizon B in relation to A. Alternatives for the improvement of the efficiency analysis and the reliability of the results obtained by CT are also discussed, and indicate good precision and adaptability of the application of this technology in Planosol (Albaqualf) studies.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162003000400019	
Editor: 	São Paulo - Escola Superior de Agricultura "Luiz de Queiroz"	
Relação: 	10.1590/S0103-90162003000400019	
Formato: 	text/html	
Fonte: 	Scientia Agricola  v.60 n.4 2003	
Fonte: 	info:eu-repo/semantics/openAccess