Data/hora: 13/06/2024 02:53:31

Provedor de dados: 	65	
País: 	Brazil	
Título: 	Comparison of microbial load in immersion chilling water and poultry carcasses after 8, 16 and 24 working hours	
Autores: 	Cavani,Ricardo; Schocken-Iturrino,Ruben Pablo; Garcia,Teresa Cristina Fernandes Lopes; Oliveira,Adriana Cássia de.	
Data: 	2010-07-01	
Ano: 	2010	
Palavras-chave: 	Poultry slaughterhouses; Chiller water microbiological load; Immersion chilling.	
Resumo: 	Poultry processing facilities are known for using a great amount of water, which is mainly used on carcasses chilling stage. In Brazil, meat regulations state that each chiller tank must be emptied, cleaned and sanitized every 8 working hours. The aim of the current study was to assess the microbial load of chiller water used in poultry immersion chilling system after 8, 16 and 24 working hours in order to evaluate the reduction of water changes and chiller sanitization. Conventional physicochemical and microbiological assays were done in water supply samples (n=69) to suppress interferences caused by freshwater addition; pre chilled (n=345) post chilled carcasses (n=345) and chiller water samples of the last stage (n=69). The results showed no significant differences on microbial load samples between the three shifts suggesting that the proposed reduction may be secure and reduces the volume of wastewater that would impact the environment, besides improving the rational use of processing time.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782010000700019	
Editor: 	Universidade Federal de Santa Maria	
Relação: 	10.1590/S0103-84782010005000115	
Formato: 	text/html	
Fonte: 	Ciência Rural  v.40 n.7 2010	
Fonte: 	info:eu-repo/semantics/openAccess