Data/hora: 12/06/2024 04:48:20

Provedor de dados: 	65	
País: 	Brazil	
Título: 	Solar Tunnel Drying: Pretreatment on drying kinetic of plum tomatoes	
Autores: 	Karaaslan,Sevil; Ekinci,Kamil; Kumbul,Barbaros Salih.	
Data: 	2019-01-01	
Ano: 	2019	
Palavras-chave: 	Drying characteristics; Tomato slices; Tunnel dryer; Mathematical modeling.	
Resumo: 	ABSTRACT:  Drying of thin layer tomato was studied using a solar tunnel dryer under the ecological conditions of Isparta, Turkey. During drying process, solar irradiation, drying air temperature, relative humidity, and air velocity were measured constantly in different parts of the dryer. Drying runs were performed using plum tomatoes, characterized by an oval shape, intense red color. The change of tomatoes mass was measured daily. The color measurements of dried products were determined at the beginning and end of experiment. In this study, the fresh tomato samples were sorted, graded, washed in water and then sliced into quarters and halves before pretreated. Sun drying behavior of half and quarter sliced tomatoes pretreated with 10% NaCl solution and non-pretreated was investigated. Results showed that the drying time for pretreated and non-pretreated samples was not significantly different. However, drying time and drying rates were affected by number of tomato slices (quarter and half). Drying characteristic curves were evaluated against thirteen mathematical models and the Midilli et al model was the best descriptive model for solar tunnel drying of thin layer tomato. Color analysis emphasized that if tomatoes are pretreated with 10% NaCl solution, they should be sliced in quarter for better quality.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782019000700203	
Editor: 	Universidade Federal de Santa Maria	
Relação: 	10.1590/0103-8478cr20180988	
Formato: 	text/html	
Fonte: 	Ciência Rural  v.49 n.7 2019	
Fonte: 	info:eu-repo/semantics/openAccess