Data/hora: 10/06/2024 02:28:34

Provedor de dados: | 65
País: | Brazil
Título: | Anaerobic co-digestion of animal manure at different waste cooking oil concentrations
Autores: | Sunada,Natália da Silva; Orrico,Ana Carolina Amorim; Orrico Junior,Marco Antonio Previdelli; Lucas Junior,Jorge de; Lopes,Walter Renato Teixeira; Schwingel,Alice Watte.
Data: | 2018-01-01
Ano: | 2018
Palavras-chave: | Digestion; Biogas; Energy recycling.
Resumo: | ABSTRACT: This study aimed to obtain the best dose of waste cooking oil inclusion for the co-digestion of substrates prepared with dairy cattle and swine manure in order to maximize solids reductions and biogas yield. Analyses of total solids (TS), volatile solids (VS), and neutral detergent fiber (NDF) were performed during the loading and unloading of digesters, while biogas yield was measured twice a week. The maximum reduction in VS (51.4%) was reached with the inclusion of up to 54.6g waste cooking oil.kg manure-1. Maximum NDF degradation occurred with inclusions of up to 69.4g waste cooking oil.kg manure-1. Inclusions of up to 64g of waste cooking oil.kg manure-1 provided specific biogas yield of 291.4 and 251.0L biogas.kg VS-1 added to substrates with swine and cattle manure, respectively. Adding oil at doses between 45.1 and 69.4g waste cooking oil kg manure-1 to substrates composed of cattle or swine manure maximizes reductions of solids and fibrous constituents and enhances specific biogas yield. Furthermore, swine manure supports higher doses of waste cooking oil.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782018000700351
Editor: | Universidade Federal de Santa Maria
Relação: | 10.1590/0103-8478cr20170517
Formato: | text/html
Fonte: | Ciência Rural  v.48 n.7 2018
Fonte: | info:eu-repo/semantics/openAccess