Data/hora: 09/06/2024 12:40:17

Provedor de dados: | 70
País: | Brazil
Título: | Air flow humidification for air-assisted boom sprayer
Autores: | Stanislavski,Wilson M.; Antuniassi,Ulisses R.; Chechetto,Rodolfo G.
Data: | 2014-02-01
Ano: | 2014
Palavras-chave: | Weather Conditions; Air-assisted Boom; Application Technology.
Resumo: | The air-assisted ground spray is fairly widespread. However, due to the unpredictable weather conditions, the operational efficiency is impaired by stops on grounds of low humidity and high temperatures. The aim of this work was to assess an air humidification method and evaluate its impact on temperature and air humidity for the air curtain of the air-assisted sprayer. With respect to relative air humidity, it has increased in 6.59%, being the maximum change when inserting 1.92 L min-1. So, it is concluded that the pipeline humidification might significantly reduce temperature and enhance air humidity. The treatments performed in this study consisted of a varied flow of a humidity device, related to weather conditions. Temperature and relative air humidity were measured at 1.0 m height from right to left of middle point of the machine, corresponding to the end of the spray boom, in the middle and end of right spray boom. The readings were also performed at three different distances from the end of the pipeline and at 0.25 and 0.50 m from that to the soil. The results show that 0.48 L min-1 in the humidification system has promoted a better efficiency in reducing air-temperature, on average 2.52 ºC when compared to the non-humidified one.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100006
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162014000100006
Formato: | text/html
Fonte: | Engenharia Agrícola  v.34 n.1 2014
Fonte: | info:eu-repo/semantics/openAccess