Data/hora: 11/06/2024 15:39:46

Provedor de dados: 	70	
País: 	Brazil	
Título: 	ENVIRONMENTAL VARIABLES AND QUALITY TOOLS APPLIED TO THE OPERATOR OF AN AGRICULTURAL MICROTRACTOR	
Autores: 	Estevam,Francisca N. de L.; Queiroz,Renata F. de; Damasceno,André F.; Silva,Rouverson P. da; Voltarelli,Murilo A.; Barbosa Filho,José A. D.	
Data: 	2019-04-01	
Ano: 	2019	
Palavras-chave: 	Operator health; Thermal load; Ergonomics.	
Resumo: 	ABSTRACT Work in the field is characterized as unstructured because it is performed in inconvenient postures, without a fixed workstation, exposing the worker directly to the sun and other inclement weather. This may interfere in the health and the performance of the activity. The objective of this work was to characterize the environment of the agricultural microtractor operator, evaluating the thermal comfort during the activity in the municipality of Quixadá, CE. A model TC14 Super Yanmar Agritech microtractor, coupled to a rotary spindle, was used. For the measurements of the environmental variables, sensors and devices were installed on the operator and in the microtractor. The experimental design adopted the assumptions of statistical quality control. Fifteen collections were done daily at different times for three consecutive days. The data obtained were indices of thermal discomfort and thermography, both of which were analyzed by sequential graphs (run charts), control graph (Xbar-R chart), and scatter plot. At all rates, the work performed proved to be inadequate, exceeding the operator's capabilities and limitations. It was concluded that the activity performed by the microtractor operator is stressful. Measures should be taken to improve working conditions without affecting the operator's health.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200208	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v39n2p208-215/2019	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.39 n.2 2019	
Fonte: 	info:eu-repo/semantics/openAccess