Data/hora: 03/06/2024 00:37:14

Provedor de dados: | 70
País: | Brazil
Título: | COMPOSTING TIME REDUCTION OF AGRO-INDUSTRIAL WASTES
Autores: | Costa,Mônica S. S. De M.; Carneiro,Leocir J.; Costa,Luiz A. De M.; Pereira,Dercio C.; Lorin,Higor E. F.
Data: | 2016-12-01
Ano: | 2016
Palavras-chave: | Environmental conditions; Inoculation; Turnings.
Resumo: | ABSTRACT The agro-industrialization of animal products has led to a significant waste generation, which has been stabilized by composting process in specialized plants. Waste stabilization time on composting depends on the handling used. 12 treatments were performed, three frequency turnings combined with two environmental conditions (with and without coverage of the composting area) and with and without commercial inoculant, whose results were submitted to multiple regression analysis. Windrows turned twice a week in the first month had adequate temperature control and stabilization time of 83.5 and 95.5 days for uncovered and covered windrows, respectively. Uncovered windrows have accelerated the process in 10 days on average, with the disadvantage of increasing nutrient losses. The weekly inoculation of Bacillus (subtilis, licheniformis and polymyxa) and Yarrowia lipolytica had no significant effect (p≥0.05).
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601206
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/1809-4430-eng.agric.v36n6p1206-1217/2016
Formato: | text/html
Fonte: | Engenharia Agrícola  v.36 n.6 2016
Fonte: | info:eu-repo/semantics/openAccess