Data/hora: 02/06/2024 12:38:03

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Designing and manufacturing of a soybean harvest residue picker	
Autores: 	Schöffel,Rubem; Boller,Walter; Walber,Márcio.	
Data: 	2015-12-01	
Ano: 	2015	
Palavras-chave: 	Ruminant feeding; Soy chaff; Agricultural machinery designing.	
Resumo: 	ABSTRACT Soy harvest matches seasons with shortage of dry matter supply for ruminant feeding in most Brazilian soy-growing areas. Agricultural machinery-producing companies must have market perception, observing new opportunities and developing equipment to meet costumers’ needs. This paper aims to design, build, and test a device to collect soybean crop residues from the combine cleaning mechanism, consisting mainly of vegetable straw (chaff), and the other plant parts (stems) remain being deposited onto the ground. For equipment designing, we made use of the architectural design methodology proposed in the reference model for the agricultural machinery development process. The equipment was designed and built following the proposed methodology, then installed and put into operation in a John Deere 1165 combine. After initial testing and few adjustments, the device showed satisfactory chaff-collecting performance. The equipment consists of a screw conveyor assembled transversely to the combine and a centrifugal fan assembled on the side. The collected chaff is dumped into a trailer towed by tractor.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601053	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-Eng.Agric.v35n6p1053-1064/2015	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.35 n.6 2015	
Fonte: 	info:eu-repo/semantics/openAccess