Data/hora: 12/06/2024 14:01:39

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Analyzing the efforts in furrow openers used in low power planters	
Autores: 	Troger,Henrique C. H.; Reis,Ângelo V. dos; Machado,Antônio L. T.; Machado,Roberto L. T.	
Data: 	2012-12-01	
Ano: 	2012	
Palavras-chave: 	Hoe opener; Traction demand; No-tillage.	
Resumo: 	The furrow openers for no-till system should be easy to penetrate the soil, generate low levels of soil mobilization and require a little traction force. Thus, the aim of this research was to compare six hoe-type furrow openers, four of industrial manufacturing and two handcrafted models, which were used in planters in the region of Pelotas, Brazil. The parameters for comparison among these furrow openers were the horizontal (Fh) and vertical (Fv) forces acting on the tip of the hoe and the cross-sectional area mobilized in the furrow. The experimental design was randomized, with six treatments (furrow openers) from T1 to T6, with four repetitions, constituted by their passage through plots of 20 x 3 m. The force data were collected by load cells and a signal conditioner. The determination of the mobilized area in the furrow was done by a micro soil profilometer. It was concluded that the furrow openers T1, T4 and T6 presented the lowest values of horizontal force (statistically equal and ranging between 1,034 and 1,230 N) and that T1 and T2 produced the highest vertical forces downwards (statistically identical and varying between 749 and 845 N). The furrow openers T1, T2, T4, T5 and T6 generated soil mobilization statistically equal and between 0.006993 and 0.008933 m².	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600015	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/S0100-69162012000600015	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.32 n.6 2012	
Fonte: 	info:eu-repo/semantics/openAccess