Data/hora: 09/06/2024 14:36:20

Provedor de dados: | 86
País: | Brazil
Título: | Porous cup shape and installation mode influencing determinations of matric potential by tensiometers
Autores: | Franco,Hélio Henrique Soares; Silva,Alvaro Pires da; Tormena,Cássio Antonio; Ferreira,Camila Jorge Bernabé; Nunes,Márcio Renato; Lima,Renato Paiva de; Libardi,Paulo Leonel.
Data: | 2017-12-01
Ano: | 2017
Palavras-chave: | Puncture tensiometers; Rounded porous cup; Soil mud.
Resumo: | Abstract: The objective of this work was to determine the measurement accuracy of the soil water matric potential (ψm) by puncture tensiometers with either rounded or pointed porous cups, installed with or without “soil mud”, and to compare the performance of these tensiometers with that of tensiometers equipped with mercury manometers. The experiment was conducted in a Ultisol, in a randomized complete block design, in a factorial arrangement with five replicates. Puncture tensiometers with rounded porous cups, installed with “soil mud”, present more elevated accuracy for ψm determination in a wider measurement range, resembling tensiometers equipped with mercury manometers in drying soil.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2017001201291

Editor:

Embrapa Secretaria de Pesquisa e Desenvolvimento

Pesquisa Agropecuária Brasileira

Relação: | 10.1590/s0100-204x2017001200019
Formato: | text/html
Fonte: | Pesquisa Agropecuária Brasileira  v.52 n.12 2017
Fonte: | info:eu-repo/semantics/openAccess