Data/hora: 10/06/2024 19:14:05

Provedor de dados: 	90	
País: 	Brazil	
Título: 	Numerical modeling of the effect of variation of boundary conditions on vadose zone hydraulic properties	
Autores: 	Leão,Tairone Paiva; Gentry,Randall.	
Data: 	2011-02-01	
Ano: 	2011	
Palavras-chave: 	Numerical model; Hydrus 1D; Uncertainty; Boundary conditions; Hydraulic conductivity; Soil physics.	
Resumo: 	An accurate estimation of hydraulic fluxes in the vadose zone is essential for the prediction of water, nutrient and contaminant transport in natural systems. The objective of this study was to simulate the effect of variation of boundary conditions on the estimation of hydraulic properties (i.e. water content, effective unsaturated hydraulic conductivity and hydraulic flux) in a one-dimensional unsaturated flow model domain. Unsaturated one-dimensional vertical water flow was simulated in a pure phase clay loam profile and in clay loam interlayered with silt loam distributed according to the third iteration of the Cantor Bar fractal object Simulations were performed using the numerical model Hydrus 1D. The upper and lower pressure heads were varied around average values of -55 cm for the near-saturation range. This resulted in combinations for the upper and lower constant head boundary conditions, respectively, of -50 and -60 cm, -40 and -70 cm, -30 and -80 cm, -20 and -90 cm, and -10 and -100 cm. For the drier range the average head between the upper and lower boundary conditions was set to -550 cm, resulting in the combinations -500 and -600 cm, -400 and -700 cm, -300 and -800 cm, -200 and -900 cm, and -100 and -1,000 cm, for upper and lower boundary conditions, respectively. There was an increase in water contents, fluxes and hydraulic conductivities with the increase in head difference between boundary conditions. Variation in boundary conditions in the pure phase and interlayered one-dimensional profiles caused significant deviations in fluxes, water contents and hydraulic conductivities compared to the simplest case (a head difference between the upper and lower constant head boundaries of 10 cm in the wetter range and 100 cm in the drier range).	
Tipo: 	Info:eu-repo/semantics/report	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832011000100025	
Editor: 	Sociedade Brasileira de Ciência do Solo	
Relação: 	10.1590/S0100-06832011000100025	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Ciência do Solo  v.35 n.1 2011	
Fonte: 	info:eu-repo/semantics/openAccess