Data/hora: 11/06/2024 02:31:22

Provedor de dados: | 90
País: | Brazil
Título: | Increase of grain and green matter of corn by liming
Autores: | Ernani,P. R.; Nascimento,J. A. L.; Oliveira,L. C.
Data: | 1998-06-01
Ano: | 1998
Palavras-chave: | Liming; Corn; Silage; Acid soils; PH.
Resumo: | Despite the fact that aluminum toxicity to crops is eliminated near soil water pH of 5.5, lime recommendation in many regions aims to increase soil pH up to 6.0 or even higher. For highly buffered soils, high rates of limestone are required to raise the pH from 5.5 to 6.0, resulting in additional, sometimes unnecessary, costs. The objective of this study was to evaluate the effect of soil pH on corn yield in a very acid Hapludox. The experiment was carried out in Lages, Southern Brazil, from 1992 to 1996. The soil had water pH of 4.7, Al3+ of 33 mmol c kg-1, O.M. of 45 g kg-1 and lime requirement to pH 6.0 of 9.0 t ha-1. Dolomitic limestone at rates of 0, 4.5, 9.0, 13.5 and 18.0 t ha-1 (equivalent to pure CaCO3) was incorporated into the soil down to 17 cm depth, in 1992. Liming increased linearly the values of soil pH (from 4.7 to 6.6) and Ca and Mg, eliminated Al3+ with rates of 9.0 t ha-1 or higher, decreased slightly Al-CuCl2, Fe and Cu, and did not affect Zn and Mn. Maximum average corn yield for grain (7.9 t ha-1) and for green matter for silage (GM) (59 t ha-1) was obtained, respectively, at soil pH of 6.0 (12 t ha-1 of limestone) and of 6.1 (14 t ha-1 of limestone); maximum economic efficiency for grain was obtained at pH 5.6 (7.5 t ha-1 of limestone). Maximum yield increments due to liming were 17% for grain and 20% for GM.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06831998000200013
Editor: | Sociedade Brasileira de Ciência do Solo
Relação: | 10.1590/S0100-06831998000200013
Formato: | text/html
Fonte: | Revista Brasileira de Ciência do Solo  v.22 n.2 1998
Fonte: | info:eu-repo/semantics/openAccess