Data/hora: 03/06/2024 11:22:53

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Aggregate stability and penetration resistance after mobilization of a dystrocohesive Ultisol	
Autores: 	Tavares,Uilka E.; Rolim,Mario M.; Simões Neto,Djalma E.; Pedrosa,Elvira M. R.; Magalhães,Adriana G.; Silva,Ênio F. de F. e.	
Data: 	2017-11-01	
Ano: 	2017	
Palavras-chave: 	Furrowing; Harrowing; Soil resistance.	
Resumo: 	ABSTRACT Evaluation of mobilized soil profiles can provide important information on soil compaction reduction processes. In this context, the objective of this study was to evaluate alterations in soil penetration resistance and the impact on the aggregate stability of a cohesive Ultisol cultivated with sugarcane. The experiment was carried out at the Carpina Sugarcane Experimental Station (EECAC/UFRPE), located in the city of Carpina, PE. Penetration resistance, mobilized area and depth, and percentage of soil aggregates were evaluated before and after soil tillage. Soil mobilization improved soil aggregate uniformity and decreased penetration resistance in the 0-0.20 m layer. Coarse soil fraction, moisture and organic carbon positively contributed to the increase in soil mobilization.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001100752	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v21n11p752-757	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.21 n.11 2017	
Fonte: 	info:eu-repo/semantics/openAccess