Data/hora: 10/06/2024 02:28:21

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Agronomic performance of canola submitted to desiccation with herbicides at different maturation stages	
Autores: 	Rosa,Willian B.; Duarte Júnior,José B.; Perego,Ivonei; Almeida,Bruno H. de; Costa,Antonio C. T. da; Tomm,Gilberto O.	
Data: 	2019-06-01	
Ano: 	2019	
Palavras-chave: 	Harvest antecipation; Grain yield; Oil content.	
Resumo: 	ABSTRACT Uneven maturation in canola is an important challenge for its management in regions subject to frost and high rainfall at the end of the cycle. In order to identify practices to maximize grain yield under these growing conditions, this work evaluated the effects of desiccation with herbicides at different phenological stages on Hyola 433, one of the most commonly used hybrids in Brazil. The experiment was conducted in a randomized block design with four repetitions in a 6 x 4 factorial scheme, with five herbicides: paraquat, diquat and ammonium glufosinate at dose of 400 g a.i. ha-1, glyphosate at 1,440 g a.i. ha-1 and saflufenacil at 70 g a.i. ha-1, plus the control, at four phenological stages of silique maturation (G2, G3, G4 and G5). Desiccation at G2 and G3 reduced the oil content and thousand-grain weight on average by 60%, affecting directly grain yield. Desiccation at G4, regardless of herbicide, did not influence thousand-grain weight and oil content, but the use of diquat reduced canola yield by 187 kg ha-1. In the desiccation at G5, none of the herbicides led to differences compared to the control for thousand-grain weight, yield and oil content, and it allowed harvest to be brought forward by five days. In general, the crop presents adequate responses to the desiccation with different herbicides at the phenological stages G4 and G5.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662019000600419	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v23n6p419-424	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.23 n.6 2019	
Fonte: 	info:eu-repo/semantics/openAccess