Data/hora: 10/06/2024 06:38:10

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Drying kinetics of atemoya pulp	
Autores: 	Galdino,Plúvia O.; Figueirêdo,Rossana M. F. de; Queiroz,Alexandre J. de M.; Galdino,Pablícia O.	
Data: 	2016-07-01	
Ano: 	2016	
Palavras-chave: 	Annona cherimoya Mill. x Annona squamosa L.; Dehydration; Modeling.	
Resumo: 	ABSTRACT This study was conducted in order to obtain drying curves of whole atemoya pulp through the foam-mat drying method. The suspension was prepared with whole atemoya pulp mixed with 2% of Emustab® and 2% of Super Liga Neutra® with mixing time of 20 min, and dried in a forced-air oven at different temperatures (60; 70 and 80 °C) and thicknesses of the foam layer (0.5, 1.0 and 1.5 cm). The drying rate curves were plotted against the water content ratio and the semi-theoretical models of Henderson &amp; Pabis, Page and Midilli were used. All tested models showed coefficient of determination (R2) above 0.993, and the Midilli model showed the best fit for all conditions. Drying curves were affected by temperature and layer thickness.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016000700672	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v20n7p672-677	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.20 n.7 2016	
Fonte: 	info:eu-repo/semantics/openAccess