Data/hora: 10/06/2024 14:14:02

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Adjustment of mathematical models and quality of soybean grains in the drying with high temperatures	
Autores: 	Coradi,Paulo C.; Fernandes,Carlos H. P.; Helmich,Jean C.	
Data: 	2016-04-01	
Ano: 	2016	
Palavras-chave: 	Dimensioning; Optimization; Post-harvest.	
Resumo: 	ABSTRACT The aim of this study was to evaluate the influence of the initial moisture content of soybeans and the drying air temperatures on drying kinetics and grain quality, and find the best mathematical model that fit the experimental data of drying, effective diffusivity and isosteric heat of desorption. The experimental design was completely randomized (CRD), with a factorial scheme (4 x 2), four drying temperatures (75, 90, 105 and 120 ºC) and two initial moisture contents (25 and 19% d.b.), with three replicates. The initial moisture content of the product interferes with the drying time. The model of Wang and Singh proved to be more suitable to describe the drying of soybeans to temperature ranges of the drying air of 75, 90, 105 and 120 °C and initial moisture contents of 19 and 25% (d.b.). The effective diffusivity obtained from the drying of soybeans was higher (2.5 x 10-11 m2 s-1) for a temperature of 120 °C and water content of 25% (d.b.). Drying of soybeans at higher temperatures (above 105 °C) and higher initial water content (25% d.b.) also increases the amount of energy (3894.57 kJ kg-1), i.e., the isosteric heat of desorption necessary to perform the process. Drying air temperature and different initial moisture contents affected the quality of soybean along the drying time (electrical conductivity of 540.35 µS cm-1g-1); however, not affect the final yield of the oil extracted from soybean grains (15.69%).	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016000400385	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v20n4p385-392	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.20 n.4 2016	
Fonte: 	info:eu-repo/semantics/openAccess