Data/hora: 02/06/2024 16:39:51

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Performance of a variable-rate distribution system for simultaneous fertilizer application	
Autores: 	Barros,Murilo M. de; Volpato,Carlos E. S.; Silva,Fabio M. da; Conceição,Fagner G. da; Corrêa Júnior,Delorme; Ribeiro,Luiz F.	
Data: 	2016-02-01	
Ano: 	2016	
Palavras-chave: 	Coffee production; Precision agriculture; Application at variable doses.	
Resumo: 	ABSTRACT The objective of this study was to evaluate the performance of a variable-rate fertilizer distribution system for coffee crop, simultaneously applying two products. Two types of tests were performed: transversal deposition and longitudinal deposition. The transversal deposition test, with tarps, aimed to quantify the variations between programmed and applied doses, using a completely randomized design (CRD), in a factorial scheme, and the Scott-Knott test at p &lt; 0.05. The longitudinal deposition test aimed to determine the distribution characteristics of the equipment along the displacement line, based on relative frequency values. In addition, the application rates on both sides of the distribution system were analysed using a CRD and the Scott-Knott test at p &lt; 0.05. The application variation in the transversal deposition test with tarps was 1.59%. The variable-rate distribution system remained stable regarding the longitudinal deposition, regardless of any interaction.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016000200188	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v20n2p188-192	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.20 n.2 2016	
Fonte: 	info:eu-repo/semantics/openAccess