Data/hora: 10/06/2024 09:07:04

Provedor de dados: | 91
País: | Brazil
Título: | Tifton grass yield on constructed wetland used for swine wastewater treatment
Autores: | Matos,Antonio T.; Freitas,Wallisson S.; Martinez,Mauro A.; Tótola,Marcos R.; Azevedo,Aristéa A.
Data: | 2010-05-01
Ano: | 2010
Palavras-chave: | Cynodon dactylon Pers; Wetland systems; Animal feed.
Resumo: | It is the purpose of this study to evaluate the agronomic behavior and yield of the Tifton 85 grass (Cynodon dactylon Pers), when used in the treatment of swine wastewater (SW) with constructed wetland systems (CWs). For this purpose, five tanks were built measuring 24 x 1.1 x 0.7 m, damp-sealed with PVC canvas and filled with 0.4 m crushed stone. In two of these tanks, Tifton grass was cultivated: one of the tanks (CW 3) contained the grass, and in the other (CW4) the grass was only cultivated in the final third part of the tanks, being preceded by Alternanthera (Althernanthera philoxeroides) and cattail (Thypha latifolia L.). The SW was previously treated by means of a filtration process that consists of 0.7 m - high organic filters; the filtering beds were made of chopped sugarcane bagasse. The filter effluents were applied to CWs at a 0.8 m³ d-1 flow rate, corresponding to a hydraulic detention time of about 4.8 days. During the experimental period, three cuttings were done in CWs plants in order to evaluate the dry matter yield and the nutrient extraction capacity. All plants showed satisfactory performance in dry mass yield (86.3 and 65.3 t ha-1, in CW3 and CW4 respectively) and nutrient extraction, as well as in dry matter yield. Except for the case of Zn, the cultivation of other vegetable species in the same tank did not alter the capacity of the Tifton 85 grass extraction of the SW macro and micronutrients removal.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662010000500008
Editor: | Departamento de Engenharia Agrícola  - UFCG
Relação: | 10.1590/S1415-43662010000500008
Formato: | text/html
Fonte: | Revista Brasileira de Engenharia Agrícola e Ambiental  v.14 n.5 2010
Fonte: | info:eu-repo/semantics/openAccess