Data/hora: 13/06/2024 02:28:02

Provedor de dados: | 91
País: | Brazil
Título: | Simulation of oat development cycle by photoperiod and temperature
Autores: | Mantai,Rubia D.; Silva,José A. G. da; Marolli,Anderson; Mamann,Ângela T. W. de; Sawicki,Sandro; Krüger,Cleusa A. M. B.
Data: | 2017-01-01
Ano: | 2017
Palavras-chave: | Avena sativat; Succession system; Nitrogen; WE-Streck model.
Resumo: | ABSTRACT The simulation of oat development cycle can be used in the planning of agricultural practices. The aim of the study was to simulate and validate the duration of oat development cycle by photoperiod, temperature and coefficients of development of wheat for use in the WE-Streck model, considering different doses of N-fertilizer and systems of succession of high and low C/N ratio. The study was conducted in 2015 in a randomized block design with four replicates in a 4 x 2 factorial scheme, corresponding to N rates (0, 30, 60 and 120 kg ha-1) and oat cultivars (Barbarasul and Brisasul), respectively, in the soybean/oat and maize/oat systems. The duration of the stages from emergence to anthesis and from anthesis to maturation of oats was simulated in the WE-Streck model. The minimum, optimum and maximum temperatures that effectively simulate the oat development cycle were 4, 22 and 30 °C from emergence to anthesis and 15, 25 and 35 °C from anthesis to maturation, respectively. The intermediate-cycle oat development was efficiently simulated by the WE-Streck model using coefficients developed for wheat, with vegetative and reproductive cycles estimated at 89 and 43 days, respectively.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000100003
Editor: | Departamento de Engenharia Agrícola  - UFCG
Relação: | 10.1590/1807-1929/agriambi.v21n1p3-8
Formato: | text/html
Fonte: | Revista Brasileira de Engenharia Agrícola e Ambiental  v.21 n.1 2017
Fonte: | info:eu-repo/semantics/openAccess