Data/hora: 11/06/2024 01:24:04

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Sediment production and soil water infiltration under different simulated rainfall characteristics	
Autores: 	Almeida,Wilk S. de; Carvalho,Daniel F. de; Pereira,Fernandes A. C.; Rouws,Janaína R. C.	
Data: 	2019-08-01	
Ano: 	2019	
Palavras-chave: 	Erosivity; Rainfall intensity; Rainfall duration; Surface runoff.	
Resumo: 	ABSTRACT The study was carried out to evaluate sediment production, water infiltration and surface runoff in an Ultisol under simulated rainfalls with similar erosivity, but different combinations of intensity (Int) and duration (Dur). The rainfalls were applied after soil tillage in the period from August to September 2017, in Seropédica, RJ State, Brazil. Using a computer program, the treatments were defined from the erosivity calculated for a rainfall with intensity of 60 mm h-1 and duration of 60 min, resulting in the other combinations of Int and Dur: 44.5 mm h-1 and 106 min; 53.5 mm h-1 and 78 min; 66.9 mm h-1 and 48 min; and 76.5 mm h-1 and 38 min, in a completely randomized design with five repetitions. Sediment production varied from 2.17 to 6.11 g m-2, respectively, in the treatments with Int 53.5 mm h-1 and Dur 78 min and Int 44.5 mm h-1 and Dur 106 min. Stable infiltration rate (mm h-1) were 21.6, 37.7, 31.4, 29.5, and 22.4, respectively, in the treatments Int 44.5 mm h-1 and Dur 106 min; Int 53.5 mm h-1 and Dur 78 min; Int 60.4 mm h-1 and Dur 60 min; Int 66.9 mm h-1 and Dur 48 min; and Int 76.5 mm h-1 and Dur 38 min. The different combinations of intensity and duration of rainfalls with similar erosivity change sediment production, but do not significantly influence surface runoff and water infiltration in the soil.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662019000800572	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v23n8p572-578	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.23 n.8 2019	
Fonte: 	info:eu-repo/semantics/openAccess