Data/hora: 12/06/2024 09:27:34

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Yield and water use of cherry tomato under water availability and potassium doses	
Autores: 	Pacheco,Adriano B.; Silva,Tonny J. A. da; Bonfim-Silva,Edna M.; Castro,Hamilton A. W.; Koetz,Marcio.	
Data: 	2018-05-01	
Ano: 	2018	
Palavras-chave: 	Lycopersicon esculentum Mill.; Available water; Potassium fertilization.	
Resumo: 	ABSTRACT The objective of this study was to evaluate the yield and water use of cherry tomatoes under soil water availability and potassium (K) doses in a greenhouse. The experiment was conducted in randomized blocks in a 52 fractional factorial design, corresponding to five levels of water availability and five K doses, with 13 combinations (4-0; 4-250; 4-500; 14-125; 14-375; 24-0; 24-250; 24-500; 34-125; 34-375; 44-0; 44-250; 44-500) (kPa-mg dm-3) and four replicates. A drip irrigation system with semi-automated irrigation control was used. The analyzed variables were shoot dry matter, number of fruits, yield, water consumption and water use efficiency. Highest cherry tomato yield occurs at soil water tension of 24 kPa and K dose of 290 mg dm-3. Soil water tension of 44 kPa and K dose of 290 mg dm-3 allow for higher water use efficiency in cherry tomato. Cherry tomato yield and water use are influenced by soil water availability and K doses in greenhouse.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662018000500326	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v22n5p326-331	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.22 n.5 2018	
Fonte: 	info:eu-repo/semantics/openAccess