Data/hora: 06/06/2024 05:39:08

Provedor de dados: | 96
País: | Brazil
Título: | Potential of biogas and methane production from anaerobic digestion of poultry slaughterhouse effluent
Autores: | Sunada,Natália da Silva; Orrico,Ana Carolina Amorim; Orrico Júnior,Marco Antônio Previdelli; Vargas Junior,Fernando Miranda de; Garcia,Rodrigo Garófallo; Fernandes,Alexandre Rodrigo Mendes.
Data: | 2012-11-01
Ano: | 2012
Palavras-chave: | Chemical oxygen demand; Total solids; Volatile solids.
Resumo: | The objective of this study was to evaluate the efficiency of anaerobic digestion on the treatment of effluent from poultry slaughterhouse. The experiment was conducted at the Laboratory of Waste Recycling from Animal Production/FCA/UFGD. During four weeks, eight experimental digesters, semi-continuous models, were loaded and set according to the hydraulic retention time (HRT) of 7, 14, 21 and 28 days, and according to the solid fraction treatment, separated with 1 mm sieve or without separation. The average weekly production of biogas and methane as well as the methane concentrations, the potential production per amount of chemical oxygen demand (COD) added and reduced, the concentrations of N, P and K at the beginning and end of process, and the most likely numbers of total and thermotolerant coliforms were evaluated. For data analysis, a completely randomized design was performed in a 4 × 2 factorial arrangement (4 HRT: 7, 14, 21 and 28 days and separation with 1 mm sieve or without separation), with repetition over time. The highest production of biogas and methane was statistically significant for the HRT of 7 and 14 days (5.29 and 2.38 L of biogas and 4.28 and 1.73 L of methane, respectively). There was an interaction between HRT and the separation of the solid with sieve and the highest production was obtained in the treatment without separation. Similar behavior was observed for the potential production with a maximum of 0.41 m³ methane.kg-1 COD added with an HRT of 7 days without separation of the solid fraction. The separation of the solid fraction is not recommended in the pretreatment of liquid effluent from poultry slaughterhouse, once the potential for production and production of methane and biogas were reduced with this treatment.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982012001100013
Editor: | Sociedade Brasileira de Zootecnia
Relação: | 10.1590/S1516-35982012001100013
Formato: | text/html
Fonte: | Revista Brasileira de Zootecnia  v.41 n.11 2012
Fonte: | info:eu-repo/semantics/openAccess