Consulta: creatorFacets:"Almeida,Brivaldo Gomes de"
Registros recuperados: 3
Data/hora: 10/06/2024 19:15:14

Improvement of a testing apparatus for dynamometry: procedures for penetrometry and influence of strain rate to quantify the tensile strength of soil aggregates
Provedor de dados: 90
Autores: Figueiredo,Getulio Coutinho; Silva,Alvaro Pires da; Tormena,Cássio Antonio; Giarola,Neyde Fabíola Balarezo; Moraes,Sergio Oliveira; Almeida,Brivaldo Gomes de.
Soil penetration resistance (PR) and the tensile strength of aggregates (TS) are commonly used to characterize the physical and structural conditions of agricultural soils. This study aimed to assess the functionality of a dynamometry apparatus by linear speed and position control automation of its mobile base to measure PR and TS. The proposed equipment was used for PR measurement in undisturbed samples of a clayey "Nitossolo Vermelho eutroférrico" (Kandiudalfic Eutrudox) under rubber trees sampled in two positions (within and between rows). These samples were also used to measure the volumetric soil water content and bulk density, and determine the soil resistance to penetration curve (SRPC). The TS was measured in a sandy loam "Latossolo Vermelho...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Soil physical quality; Tensile stress; Soil penetration resistance.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832011000200008

Desenvolvimento de um consolidômetro pneumático: modelagem da compactação, penetrometria e resistência tênsil de agregados de solo
Provedor de dados: 90
Autores: Figueiredo,Getulio Coutinho; Silva,Alvaro Pires da; Tormena,Cássio Antonio; Giarola,Neyde Fabíola Balarezo; Moraes,Sergio Oliveira; Almeida,Brivaldo Gomes de.
A compactação é um dos processos responsáveis pela degradação física do solo que pode ocasionar a perda da sustentabilidade da produção agrícola. Assim, é fundamental dispor de estratégias instrumentais para quantificar as propriedades físicas que são influenciadas pela compactação e utilizadas para avaliar a qualidade do solo. Os objetivos deste trabalho foram: desenvolver um consolidômetro com propulsão pneumática de baixo custo; avaliar sua funcionalidade mediante estudo do comportamento compressivo de um Latossolo Vermelho distrófico de textura argilo-arenosa sob plantio direto; e avaliar o potencial de utilização da propulsão pneumática para determinações de resistência do solo à penetração (RP) e de resistência tênsil de agregados (RT). A avaliação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ensaio de compressão uniaxial; Pressão de preconsolidação; Índice de compressão; Resistência do solo à penetração; Estresse tênsil.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832011000200009

Structural quality of polyacrylamide-treated cohesive soils in the coastal tablelands of Pernambuco
Provedor de dados: 90
Autores: Melo,Diego Vandeval Maranhão de; Almeida,Brivaldo Gomes de; Souza,Edivan Rodrigues de; Silva,Laércio Santos; Jacomine,Paulo Klinger Tito.
Water-soluble polymers are characterized as effective flocculating agents due to their molecular features. Their application to soils with horizons with structural problems, e.g, a cohesive character, contributes to improvements in the physical quality and thus to the agricultural suitability of such soils. The purpose of this study was to evaluate the structural quality of soils with cohesive horizons of coastal tablelands in the State of Pernambuco treated with polyacrylamide (PAM) as chemical soil conditioner. To this end, three horizons (one cohesive and two non-cohesive) of a Yellow Argisol (Ultisol) were evaluated and to compare cohesive horizons, the horizon of a Yellow Latosol (Oxisol) was selected. The treatments consisted of aqueous PAM solutions...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anionic polymer; Coagulation/flocculation; Aggregate stability.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832014000200012