Consulta: creatorFacets:"Bassoullet, Philippe"
Registros recuperados: 15
Data/hora: 07/06/2024 00:29:50

Hydrosedimentological processes and soils of the barito estuary (south-kalimantan, indonesia)
Provedor de dados: 5
Autores: Bassoullet, Philippe; Djuwansah, R; Gouleau, D; Marius, C.
A pluridisciplinary study was carried out in the south-eastern part of Kalimantan (Indonesia) in a deltaic area close to Banjarmasin town. Upstream from Banjarmasin, Barito river divides into two branches, one of which meets the Kapuas river slightly further to the west, to form the Kapuas Murung estuary. This programme is designed to increase knowledge about the physical and sedimentological processes, physical and chemical properties of the soils, and hydrological and chemical parameters of the Barito estuary. Barito estuary was chosen for two main reasons. First, it constitutes an important waterway for the region, on which Banjarmasin harbour is located; second, the management of the sparsely occupied coastal areas is becoming a priority. The...
Tipo: Text
Ano: 1986
URL: http://archimer.ifremer.fr/doc/00110/22110/19748.pdf

Golfe Normano-Breton - Etude Régionale Intégrée
Provedor de dados: 5
Autores: Le Hir, Pierre; Bassoullet, Philippe; Erard, E.; Blanchard, Michel; Hamon, Dominique; Jegou, Anne-marie.
Ce rapport en 6 volumes est le résultat d'une étude pluridisciplinaire (6 thèmes correspondant aux volumes du rapport), réalisée sur un secteur géographique bien délimité, présentant des caractéristiques physiques et biologiques particulières (très fort marnage, grande hétérogénéité des fonds, forte production biologique à base de mollusques filtreurs…), et siège d'activités humaines importantes et diversifiées (essentiellement basées sur l'exploitation des ressources du milieu). L'étude fait suite à un Livre Blanc établi en 1982, synthétise les données existantes, et les complète par des travaux originaux sur la connaissance des mécanismes naturels, en particulier de ceux qui ont une relation directe ou indirecte avec les activités humaines (processus...
Tipo: Text
Ano: 1986
URL: http://archimer.ifremer.fr/doc/00047/15837/13240.pdf

Modélisation hydro-sédimentaire de la baie du Mont Saint-Michel
Provedor de dados: 5
Autores: Cayocca, Florence; Dussauze, Morgan; Le Hir, Pierre; Bassoullet, Philippe; Jestin, Herve.
A numerical model for hydrodynamics and sediment transport is applied to Mont Saint Michel Bay, where ecological concerns are related to sediment transfers. Recent current datasets recorded on the tidal flat show the wind influence on the currents during neap tide. They are compared to model outputs. The simulation of sediment transfers driven by tides and waves accurately mimics the sediment repartition in the Bay.
Tipo: Text
Palavras-chave: Turbidité; Sédiments cohésifs; Modèle; Courant; Mont Saint Michel.
Ano: 2006
URL: http://archimer.ifremer.fr/doc/2006/acte-6274.pdf

Remaniements sédimentaires superficiels sur l'estran occidental de la baie du Mont Saint-Michel
Provedor de dados: 5
Autores: Bonnot-courtois, C; Bassoullet, Philippe; Tessier, B; Cayocca, Florence; Le Hir, Pierre; Baltzer, A.
In order to define and quantify the rhythm and amplitude of the processes of erosion and sedimentation on broad tidal flats, in situ measurements of sediment elevation have been performed in the western part of the Mont-Saint-Michel bay. The amplitude of reworking is generally low (&lt; ± 5 cm), and variable from west to east. The wind influence on tidal currents and surficial reworking emphasizes erosion phases rapidly followed by accretion of similar amplitude on the whole tidal flat. A numerical model for hydrodynamics and sediment transport is applied to Mont Saint Michel Bay, where ecological concerns are related to sediment transfers.
Tipo: Text
Palavras-chave: Sediment transport; Numerical model; Erosion sedimentation budget; "In situ" measurements; Tidal sandy mud flat; Transport sédimentaire; Modèle numérique; Bilan érosion sédimentation; Mesures in situ; Estran sablo vaseux.
Ano: 2008
URL: http://archimer.ifremer.fr/doc/2008/publication-6279.pdf

Dragages et environnement marin Etat des connaissances
Provedor de dados: 5
Autores: Alzieu, Claude; Abarnou, Alain; Bassoullet, Philippe; Boutier, Bernard; Chiffoleau, Jean-francois; Crenn, Isabelle; Derrien, Annick; Erard-le Denn, Evelyne; Gourmelon, Michele; Guiliaud, Jean-françois; Silva Jacinto, Ricardo; Le Cann, Pierre; Le Guyader, Françoise; Le Hir, Pierre; L'Yavanc, Jacky; Mauvais, Jean-louis; Menard, Dominique; Michel, Pierre; Monbet, Yves; Pommepuy, Monique; Quiniou, Francoise.
Port activities require continuous or occasional dredging of considerable quantities of sediments : approximately 50 million m3 along the French coastline. A large proportion of the dredgings is authorized for dumping at sea in geographically delimited areas and following an impact evaluation of their potential harmfulness to the marine environment. The environmental risks assessment linked to dredging operations relies on knowledge related to several scientific disciplines contributing to changes in the regulations. This work, intended both for managers and for environmental scientists and engineers, is designed to take stock of the current state-of-the-art in the field of sediment contamination and related ecotoxicological hazards, along with a review of...
Tipo: Text
Palavras-chave: Regulations; Management; Impact; Contaminants; Dredging; Réglementation; Gestion; Impact; Contaminants; Dragages.
Ano: 1999
URL: http://archimer.ifremer.fr/doc/1999/rapport-1040.pdf

Réalisation d'un modèle de dispersion d'un rejet de dragage et des contaminants associés. Rapport définitif: contrat « LITEAU » 2ème phase
Provedor de dados: 5
Autores: Alzieu, Claude; Andral, Bruno; Bassoullet, Philippe; Boutier, Bernard; Gonzalez, Jean-louis; Huet, Martial; Jestin, Herve; L'Yavanc, Jacky; Michel, Pierre; Paulet, Yves-marie; Quiniou, Francoise; Silva Jacinto, Ricardo.
Le projet à pour but de modéliser la dispersion des immersions des boues de dragage, à partir de modèles numériques de manière à pouvoir évaluer le devenir de la charge particulaire et des contaminants associés. Les résultats des expérimentations en laboratoire montrent, qu'à l'échelle représentative du temps de séjour des particules dans la colonne d'eau du champ proche (quelques heures), on ne constate pas de solubilisation des métaux. La libération de la fraction associée aux eaux interstitielles et les flux à l'interface eau-sédiment (diagenèse précoce) après dépôt des sédiments rejetés, sont les processus qui pourraient être la cause d'un apport important de Cd (ou autre contaminant) dissous dans le milieu. Les hypothèses retenues pour l'élaboration...
Tipo: Text
Ano: 2003
URL: http://archimer.ifremer.fr/doc/00075/18621/16172.pdf

Rejets urbains. Volet Manche - Atlantique - Site de Morlaix - Etudes sédimentologique et Bathymétrique de l' estuaire de Morlaix
Provedor de dados: 5
Autores: Bassoullet, Philippe; L'Yavanc, Jacky; Guillaud, Jean-francois; Loarer, Ronan; Breton, Marguerite.
In order to increase our knowledge about sediment transport in the bay and maritime part of the River of Morlaix (Finistère), measurernènts have been perforrned on site. This report gives the granulometrical and physical parameters of the sediments as weIl as the hydrodynamics, used for a model of particulate transport in the area. The rnodel and its application will be published later
Tipo: Text
Palavras-chave: Rejet urbain; Sédiment; Granulométrie; Hydrodynamique; Modèle de transport particulaire; Sable; Vase; Estuaire de Morlaix.; Urban wastes; Model; Sediment; Granulometry; Hydrodynamics; Sand; Mud; Sedimentary transport model; Morlaix estuary.
Ano: 1987
URL: http://archimer.ifremer.fr/doc/00345/45658/45293.pdf

Modelling mud transport in a macrotidal estuary
Provedor de dados: 5
Autores: Le Hir, Pierre; Bassoullet, Philippe; L'Yavanc, Jacky.
In order to determine the fate of the fine particles and adsorbed contaminants in·a short macrotidal èstuary, a mathematical modelling system for cohesive suspended mater transport and bottom evolution, including a new consolidation algorithm, is developed. An analysis of successive erosion, transport and deposi~ion processes due to tidal forcing is given and comparisons with field data are provided. A description of mean-term bottom variations has been attempted and is partially validated by differential soundings.
Tipo: Text
Palavras-chave: Dynamique des sédiments cohésifs; Estuaire Morlaix; Tassement des vases; Modèle mathématique; Érosion; Dépôt; Cohesive sediment dynamics; Estuary; Erosion; Deposition; SoiT consolidation; Mathematical modelling.
Ano: 1988
URL: https://archimer.ifremer.fr/doc/00682/79379/81909.pdf

Observations de l'Ifremer sur la demande d'amélioration du chenal de navigation dans l'estuaire de la Gironde
Provedor de dados: 5
Autores: Manaud, Francois; Bassoullet, Philippe; Dreves, Luc; Le Hir, Pierre; L'Yavanc, Jacky; Prouzet, Patrick; Quintin, Jean-yves.
Tipo: Text
Ano: 2003
URL: http://archimer.ifremer.fr/doc/00269/38070/36185.pdf

Analysis of mixed-sediment consolidation experiments
Provedor de dados: 5
Autores: Grasso, Florent; Le Hir, Pierre; Bassoullet, Philippe.
Estuarine sediment transport models require that a time variation of erodibility due to consolidation be taken into account. If numerical modelling of mud sedimentation and consolidation is currently satisfactory, simulation of mud-sand mixture consolidation is more problematical. This is partly due to mixed-sediment processes, as hindered settling and segregation, not well understood yet. Hence, based on extensive settling columns experiments, the aim of this study is to improve our understanding of mud-sand mixture consolidation for varying concentrations (54 to 600 kg/m3) and large sand contents (15 to 80%). Firstly, we observed that for a given initial mass concentration and sand content the final consolidation appeared independent from the initial...
Tipo: Text
Palavras-chave: Settling column experiments; Consolidation; Sedimentation; Mud/sand mixtures; Sand segregation; Gelling concentration.
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00206/31727/30129.pdf

Numerical modelling of mixed-sediment consolidation
Provedor de dados: 5
Autores: Grasso, Florent; Le Hir, Pierre; Bassoullet, Philippe.
Sediment transport modelling in estuarine environments, characterised by cohesive and non-cohesive sediment mixtures, has to consider a time variation of erodibility due to consolidation. Generally, validated by settling column experiments, mud consolidation is now fairly well simulated; however, numerical models still have difficulty to simulate accurately the sedimentation and consolidation of mixed sediments for a wide range of initial conditions. This is partly due to the difficulty to formulate the contribution of sand in the hindered settling regime when segregation does not clearly occur. Based on extensive settling experiments with mud-sand mixtures, the objective of this study was to improve the numerical modelling of mixed-sediment consolidation...
Tipo: Text
Palavras-chave: Mud-sand mixtures; Hindered settling; Consolidation; Experiments; Numerical modelling; Segregation.
Ano: 2015
URL: https://archimer.ifremer.fr/doc/00254/36539/35168.pdf

Sedimentary processes in a shellfish farming environment, Mont Saint Michel Bay, France
Provedor de dados: 5
Autores: Cayocca, Florence; Bassoullet, Philippe; Le Hir, Pierre; Jestin, Herve; Cann, Philippe.
Mont Saint Michel Bay is a 30 km wide bay located on the French side of the English Channel. The tidal range reaches 14 m during spring tides, which leads, along with the gentle slope of the bathymetry, to a tidal flat up to 11 km wide. The sedimentary coverage exhibits strong longshore and cross-shore gradients, with purely muddy environments to the west of the domain, and pure sands to the east, where the natural channels of three incoming rivers induce rapid morphological changes. The contributions of tides and waves to sedimentary processes are analysed by means of numerical modelling and results of field observations. Maximum tidal bottom shear stresses are shown to account for the sediment distribution throughout the bay, while the longshore gradient...
Tipo: Text
Ano: 2008
URL: http://archimer.ifremer.fr/doc/2008/publication-6278.pdf

Utilisation d’un altimètre (ALTUS) destiné à la quantification des dépôt/érosion en domaine littoral pour l’étude des corrélations avec les caractéristiques de vagues et les interfaces de dépôt
Provedor de dados: 5
Autores: Bassoullet, Philippe; Verney, Romaric; Kervella, Youen; Kervella, Stephane; Jestin, Herve; Voineson, Guillaume.
Quantitative evaluation of erosion/deposition events of surficial sediments is crucial to understand the processes and establish sedimentary budgets in coastal areas The ALTUS system was designed for more than a decade, to meet this objective The possibilities offered by this altimeter (short-term or several months measurements) are particularly fitted for validation of sedimentary transport numerical models The recent integration of a large capacity memory card has allowed to optimize the system Indeed it is well established that wave activity is one of the key parameters for the erosion and hence govern sediment transport in intertidal/shallow water areas The ALTUS system in addition to bottom level variation recordings allows access to wave...
Tipo: Text
Ano: 2010
URL: http://archimer.ifremer.fr/doc/00019/13036/10170.pdf

La Crépidule : identifier les mécanismes de sa prolifération et caractériser ses effets sur le milieu pour envisager sa gestion (Chantier : Baie de Saint-Brieuc)
Provedor de dados: 5
Autores: Hamon, Dominique; Blanchard, Michel; Houlgatte, Eric; Blanchet, Aline; Gaffet, Jean-dominique; Cugier, Philippe; Menesguen, Alain; Bassoullet, Philippe; Cann, Philippe; Domalain, David; Haubois, Anne-gaelle.
La crépidule (Crepidula fornicata), mollusque gastéropode de la famille des Calyptraeidés, originaire de la côte atlantique d'Amérique du nord, a été introduite accidentellement sur le littoral français en plusieurs étapes (Blanchard, 1995, 1997). La plus importante d'entre elles, au début des années 70, est liée à l'importation massive de l'huître japonaise (Crassostrea gigas), en remplacement de l'huître portugaise (Crassostrea angulata) décimée par une épizootie. Cette espèce opportuniste a notamment proliféré au voisinage des principaux bassins ostréicoles de la Manche et de l'Atlantique. C'est en particulier le cas des zones conchylicoles infralittorales du golfe normano-breton où des évaluations de stocks font état de plusieurs centaines de milliers...
Tipo: Text
Ano: 2002
URL: http://archimer.ifremer.fr/doc/00032/14295/11574.pdf

Modeling mud transport in a macrotidal estuary
Provedor de dados: 5
Autores: Le Hir, Pierre; Bassoullet, Philippe; L'Yavanc, Jacky.
In order to determine the fate of the fine particles and adsorbed contaminants in a short macrotidal estuary, a mathematical modelling system for cohesive suspended mater transport and bottom evolution, including a new consolidation algorithm, is developed. An analysis of successive erosion, transport and deposition processes due to tidal forcing is given and comparisons with field data are provided. A description of mean-terrn bottom variations has been attempted and is partially validated by differential sounding.
Tipo: Text
Ano: 1988
URL: http://archimer.ifremer.fr/doc/00080/19146/16741.pdf