Consulta: creatorFacets:"Brault, Patrice"
Registros recuperados: 6
Data/hora: 01/06/2024 08:25:10

NAOS: Profileurs Deep Arvor &amp; Argos-3 – 4ème Réunion annuelle
Provedor de dados: 5
Autores: Dutreuil, Vincent; Andre, Xavier; Le Reste, Serge; Thierry, Virginie; Renaut, Corentin; Brault, Patrice; Sagot, Jerome; David, Arnaud.
Tipo: Text
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00280/39081/37646.pdf

Le projet Equipex NAOS : l'observation globale des océans Préparation de la nouvelle décennie d'Argo
Provedor de dados: 5
Autores: Le Traon, Pierre-yves; D'Ortenzio, Fabrizio; Babin, Marcel; Claustre, Hervé; Pouliquen, Sylvie; Le Reste, Serge; Thierry, Virginie; Brault, Patrice; Guigue, Michel; Le Menn, Marc.
NAOS (Novel Argo Ocean observing System) is one of the 52 projects selected as part of the Equipex call for proposals from the French programme d'investissements d'avenir. The overall objective of the project is to consolidate and improve the French and European contribution to the international Argo observing system and to prepare the next decade of Argo. The challenge is to set up an effective monitoring of the world ocean and to strengthen French leadership in ocean and climate research and prediction.
Tipo: Text
Palavras-chave: Méthode d'observation océanographique; Réchauffement climatique; Prévision climatique; Salinité de l'eau; Température de l'eau; Océan mondial; Altimètre radar; CO2; Tempête; Cyclone tropical; Mousson; El-Niño; Circulation générale océanique; Climatologie océanographique; Modèle couplé océan-atmosphère; Modèle climatique.
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00117/22801/20608.pdf

Development and validation of the new ProvBioII float
Provedor de dados: 5
Autores: Leymarie, Edouard; Poteau, Antoine; Andre, Xavier; Besson, F; Brault, Patrice; Claustre, Herve; David, Arnaud; D'Ortenzio, Fabrizio; Dufour, A; Lavigne, Heloise; Le Reste, Serge; Le Traon, Pierre-yves; Migon, Christophe; Nogre, David; Obolensky, G; Penkerc'H, C; Sagot, Jerome; Schaeffer, Christophe; Schmechtig, C; Taillandier, V.
In the last ten years, a productive collaboration has grown between the Laboratoire d’Océanographie de Villefranche (LOV), NKE and IFREMER to implement biogeochemical sensors on profiling floats. A first project (2003) was dedicated to the design of the so-called ProvBio floats (models A and B) that consisted of a PROVOR-CTS3 float instrumented with three new optical sensors: a Wetlabs transmissometer (C-Rover), a 3-wavelength Satlantic radiometer (OCR-503) and an “ECO3” Wetlabs sensor, measuring chlorophyll-a fluorescence, colored dissolved organic matter and particle backscattering coefficients (see First Success of ProvBio floats, Coriolis Letter n°5). Then, the integration of biogeochemical sensors continued in the framework of ProNuts project (2009,...
Tipo: Text
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00219/32989/31438.pdf

NAOS : preparing the new decade for Argo
Provedor de dados: 5
Autores: Le Traon, Pierre-yves; D'Ortenzio, Fabrizio; Babin, M.; Claustre, H.; Pouliquen, Sylvie; Le Reste, Serge; Thierry, Virginie; Brault, Patrice; Guigue, Michel; Le Menn, M.
Tipo: Text
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00114/22556/20244.pdf

Deep-Arvor: The results of the first industrial prototype deployment
Provedor de dados: 5
Autores: Dutreuil, Vincent; Le Reste, Serge; Thierry, Virginie; Andre, Xavier; Lenault, Yannick; Renaut, Corentin; Brault, Patrice; Sagot, Jerome; David, Arnaud.
Deep-Arvor was designed by Ifremer to achieve more than 150 profiles from 4,000 meters depth, with CTD continuously pumping and oxygen measurements. After the validation of two first models at the sea, the industrialization has been entrusted to NKE. The first constructed prototypes of Deep-Arvor have been deployed successfully in May 2014. Thanks to its light weight, Deep-Arvor maintains the self-ballasting feature of Provor/Arvor and the easy deployment of Arvor. High resolution profiles are transmitted by the Iridium satellite system.
Tipo: Text
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00222/33347/31748.pdf

Développement et essais d’un salinomètre optique pour l’océanographie
Provedor de dados: 5
Autores: Le Menn, Monique; Malardé, Damien; David, Arnaud; Brault, Patrice; Grosso, Philippe; De Bougrenet De La Tocnaye, Jean-louis; Le Reste, Serge; Podeur, Christian.
Salinity is the essential parameter for ocean dynamics studies. Its definition and using in the equations used to calculate the thermodynamic properties of seawater, were revised in 2010, opening the possibility of new sensors developments. In this context, NOSS (NKE Optical Salinity Sensor) has emerged as one of the first underwater instrument for in situ refractive index measurement in the past years open up the scope of possibilities to access to density parameter. This achievement is the fruit of the cooperation between several institutions and the fruit of several years of developments and trials. NOSS sensor is designed to be deployed in coastal environment and open-ocean waters up to 2000m, especially on profiling floats of the Argo network.
Tipo: Text
Palavras-chave: Salinity; Density; Ocean; Seawater; Refractive index; Sensor.
Ano: 2016
URL: https://archimer.ifremer.fr/doc/00664/77601/79616.pdf