Consulta: creatorFacets:"Cruvinel,Paulo Estevão"
Registros recuperados: 3
Data/hora: 09/06/2024 07:31:11

Tomografia computadorizada aplicada a estudos de um Planossolo
Provedor de dados: 86
Autores: Pedrotti,Alceu; Pauletto,Eloy Antonio; Crestana,Silvio; Cruvinel,Paulo Estevão; Vaz,Carlos Manoel Pedro; Naime,João de Mendonça; Silva,Alvaro Macedo da.
Na busca de técnicas mais apuradas para a determinação e avaliação de parâmetros físicos do solo com aplicabilidade em várzeas, vem se destacando a tomografia computadorizada, por medir a densidade e a umidade com boa sensibilidade e alta resolução espacial. O presente trabalho teve como objetivo descrever aspectos e procedimentos da calibração de um minitomógrafo de raios-X e gama para estudo da densidade e umidade de um Planossolo no Rio Grande do Sul, bem como estabelecer parâmetros estatísticos para sua adequada utilização. A calibração do minitomógrafo foi obtida pela regressão linear entre as unidades tomográficas (UT), apresentadas pelo programa de reconstrução de imagem, e os coeficientes de atenuação linear (µl, cm-1), medidos por transmissão...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Várzea densidade do solo umidade do solo calibração; Minitomógrafo.
Ano: 2003
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2003000700005

Intelligent instrument to facilitate decision making in the evaluation of soil resistance to root penetration
Provedor de dados: 63
Autores: Rabello,Ladislau Marcelino; Cruvinel,Paulo Estevão.
This contribution introduces an instrument for decision-making in agricultural processes based on the measurements and mapping of soil resistance to root penetration. Its development was based on a new and advanced instrumentation tool, enabling in almost real-time to acquire the necessary information for spatial variability analysis of plant root penetration resistance in soils, due to natural or artificial soil compaction processes, i.e., not only for an area of soil but also for a soil profile. The system allows soil resistance assays for both laboratory and agricultural fields. Moreover, the development focused on an intelligent instrumentation concept, as well as a microprobe (30º for the spire angle, 1,6 mm for the base diameter, and 30 mm of total...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural instrumentation; Intelligent systems; Signal processing; Soil microprobe; Soil penetrometer.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162009000500001

Planosol soil sample size for computerized tomography measurement of physical parameters
Provedor de dados: 63
Autores: Pedrotti,Alceu; Pauletto,Eloy Antonio; Crestana,Silvio; Cruvinel,Paulo Estevão; Vaz,Carlos Manoel Pedro; Naime,João de Mendonça; Silva,Alvaro Macedo da.
Computerized tomography (CT) is an important tool in Soil Science for noninvasive measurement of density and water content of soil samples. This work aims to describe the aspects of sample size adequacy for Planosol (Albaqualf) and to evaluate procedures for statistical analysis, using a CT scanner with a 241Am source. Density errors attributed to the equipment are 0.051 and 0.046 Mg m-3 for horizons A and B, respectively. The theoretical value for sample thickness for the Planosol, using this equipment, is 4.0 cm for the horizons A and B. The ideal thickness of samples is approximately 6.0 cm, being smaller for samples of the horizon B in relation to A. Alternatives for the improvement of the efficiency analysis and the reliability of the results obtained...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lowland; Albaqualf; Bulk density; Compaction; Soil moisture.
Ano: 2003
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162003000400019