Consulta: creatorFacets:"Cunha, Fernando França da"
Registros recuperados: 5
Data/hora: 12/06/2024 05:03:28

DRIPPERS AND DEVICES OF LINE ENDINGS OPERATING WITH WATERS CONTAINING DIFFERENT CONCENTRATIONS OF ORGANIC MATERIAL
Provedor de dados: 107
Autores: Cunha, Fernando França da; Silva, Thiago Ramos da; Muchalak, Sofia Michele; Magalhães, Fernando Fagner; Silva, Simone Quintão.
This study aimed to evaluate the performance of a dripper and of a self-cleaning valve operating with water containing different concentrations of total solids. The experiment was conducted in sub-subplots design, having on the plots two line endings (conventional and self-cleaning valve), in the subplots five waters with total solids concentrations (7 mg L-1, 407 mg L-1, 1,007 mg L-1, 2,007 mg L-1, 4,007 mg L-1) and on the sub-subplots 60 reviews of irrigation system, on the completely randomized design with three replications. In the end of the trial period, each dripper applied a cumulative volume of 1.44 m³. The parameters evaluated were: flow and the uniformities of water applications through the distribution coefficients (DU), Christiansen (CU) and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos Hídricos e Ambientais / Irrigação Irrigação localizada; Sólidos totais; Uniformidade de aplicação.
Ano: 2017
URL: http://www.seer.ufv.br/seer/index.php/reveng/article/view/764

CARACTERÍSTICAS DA ESPIGA DO MILHO DOCE PRODUZIDO SOB DIFERENTES LÂMINAS DE IRRIGAÇÃO E DOSES NITROGENADAS
Provedor de dados: 107
Autores: Souza, Epitácio José de; Cunha, Fernando França da; Magalhães, Fernando Fagner; Silva, Thiago Ramos da; Santos, Osvaldir Feliciano dos.
Objetivou-se, neste trabalho, avaliar as características da espiga do milho doce produzido sob diferentes doses de adubação nitrogenada e lâminas de irrigação, em duas épocas de cultivo na região nordeste do Mato Grosso do Sul. O experimento foi conduzido em parcelas subsubdivididas, tendo nas parcelas quatro lâminas de irrigação (50, 75, 100 e 125% da evapotranspiração da cultura - ETc), nas subparcelas quatro doses de nitrogênio em cobertura (0, 100, 200 e 300 kg ha-1) e nas sub-subparcelas duas épocas de cultivo (Inverno/Primavera e Verão/Outono), no delineamento em blocos casualizados, com quatro repetições. Foram avaliadas as características: número de palha por espiga, comprimento de espiga, diâmetro de espiga, número de grãos por fileira, número de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos Hídricos e Ambientais / Irrigação adubação; Irrigação por gotejamento; Sazonalidade; Zea mays var. Saccharata Sturt.
Ano: 2016
URL: http://www.seer.ufv.br/seer/index.php/reveng/article/view/617

NOTA TÉCNICA: USO DO SOFTWARE INTECPERÍMETRO® NO MANEJO DA IRRIGAÇÃO DO FEIJOEIRO
Provedor de dados: 107
Autores: Ferreira, Francisco Edson Paulo; Pereira, Silvio Bueno; Martinez, Mauro Aparecido; Soares, Adilson Rodrigues; Cunha, Fernando França da.
Objetivou-se com o presente trabalho utilizar o software IntecPerímetro® na avaliação do manejo da irrigação na cultura do feijão. O software foi alimentado por dados de clima, cultura, solo e os referentes ao equipamento de irrigação. A avaliação do manejo da irrigação procedeu-se pela comparação entre os valores médios de lâmina aplicada e tempo de funcionamento do equipamento de irrigação praticados pelo irrigante e calculados por meio do uso do software IntecPerímetro® em todas as fases de desenvolvimento da cultura, por meio do teste “t” de Student ao nível de 5% de probabilidade. A lâmina média de irrigação proposta pelo software foi 28,3% menor que a praticada pelo irrigante. Os valores de umidades obtidas em campo pelo método do forno micro-ondas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos Hídricos e Ambientais / Irrigação agricultura irrigada; Hargreaves-Samani; Feijão; Pivô central.
Ano: 2016
URL: http://www.seer.ufv.br/seer/index.php/reveng/article/view/655

Multivariate adaptive regression splines (MARS) applied to daily reference evapotranspiration modeling with limited weather data
Provedor de dados: 1
Autores: Ferreira, Lucas Borges; Duarte, Anunciene Barbosa; Cunha, Fernando França da; Fernandes Filho, Elpídio Inácio.
Estimation of reference evapotranspiration (ETo) is very relevant for water resource management. The Penman-Monteith (PM) equation was proposed by the Food and Agriculture Organization (FAO) as the standard method for estimation of ETo. However, this method requires various weather data, such as air temperature, wind speed, solar radiation and relative humidity, which are often unavailable. Thus, the objective of this study was to compare the performance of multivariate adaptive regression splines (MARS) and alternative equations, in their original and calibrated forms, to estimate daily ETo with limited weather data. Daily data from 2002 to 2016 from 8 Brazilian weather stations were used. ETo was estimated using empirical equations, PM equation with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Data driven; Irrigation scheduling; Agrometeorology; Artificial intelligence.; Agrometeorologia.
Ano: 2019
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/39880

Multivariate adaptive regression splines (MARS) applied to daily reference evapotranspiration modeling with limited weather data
Provedor de dados: 1
Autores: Ferreira, Lucas Borges; Duarte, Anunciene Barbosa; Cunha, Fernando França da; Fernandes Filho, Elpídio Inácio.
Estimation of reference evapotranspiration (ETo) is very relevant for water resource management. The Penman-Monteith (PM) equation was proposed by the Food and Agriculture Organization (FAO) as the standard method for estimation of ETo. However, this method requires various weather data, such as air temperature, wind speed, solar radiation and relative humidity, which are often unavailable. Thus, the objective of this study was to compare the performance of multivariate adaptive regression splines (MARS) and alternative equations, in their original and calibrated forms, to estimate daily ETo with limited weather data. Daily data from 2002 to 2016 from 8 Brazilian weather stations were used. ETo was estimated using empirical equations, PM equation with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: 5.01.05.00-0 data driven; Irrigation scheduling; Agrometeorology; Artificial intelligence. Agrometeorologia.
Ano: 2019
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAgron/article/view/39880