Consulta: creatorFacets:"Dalri,Alexandre Barcellos"
Registros recuperados: 3
Data/hora: 09/06/2024 05:40:21

Agronomic performance of white oats cultivated under fertigation with treated sewage effluent and definition of critical limits of Normalized Difference Vegetation Index
Provedor de dados: 53
Autores: Coelho,Anderson Prates; Faria,Rogério Teixeira de; Barbosa,Aline Michelle da Silva; Dalri,Alexandre Barcellos; Rosalen,David Luciano.
ABSTRACT One of the benefits of irrigation with wastewater in agriculture is the reduction in the use of mineral fertilizers and the increase in crop yield. For wastewater application, the use of remote sensing can help to define specific management areas. The aim of this study was to evaluate the yield and the growth of irrigated white oats (Avena sativa L.) with varying treated sewage effluent (TSE) levels. These attributes were then correlated with Normalized Difference Vegetation Index (NDVI) values obtained at four phenological stages of the crop and used to define critical limits of NDVI. The experiment consisted of five TSE treatments differing in irrigation depths (11, 31, 60, 87, and 100%). Mean NDVI values in the crop were determined with an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativa L.; Biomass; Modeling; NDVI; Remote sensing.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87052019000400553

Non-pressure compensating emitters using treated sewage effluent for irrigation
Provedor de dados: 65
Autores: Fischer Filho,João Alberto; Dalri,Alexandre Barcellos; Santos,Miquéias Gomes dos; Zanini,José Renato; Faria,Rogério Teixeira de.
ABSTRACT: This study aimed to evaluate the obstruction of non-pressure compensating emitters using treated sewage effluent (TSE) for irrigation. A drip irrigation system with six models of emitters (encoded) was installed in level field conditions. TSE coming from a sewage treatment station was used as irrigation water after being filtered through a disc filter (120 mesh). Seven flow rate evaluations of drippers operating at 100kPa were performed (0, 100, 200, 300, 400, 500 and 600h of operation). The experimental design was randomized in a 6×7 factorial arrangement (6 models and 7 times), with four repetitions, and Tukey’s test was used to compare means. Relative flow rate (Qr), the flow rate coefficient of variation (CVQ) and degree of clogging (GE) were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wastewater; Trickle irrigation; Clogging; Water saving.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782017000700351

Caracterização técnica e desempenho hidráulico dequatro gotejadores autocompensantes utilizados no Brasil
Provedor de dados: 65
Autores: Dalri,Alexandre Barcellos; Garcia,Carlos Jesus Baca; Zanini,José Renato; Faria,Rogério Teixeira de; Palaretti,Luiz Fabiano.
Este trabalho teve por objetivo caracterizar e avaliar o desempenho de quatro modelos de gotejadores autocompensantes, frequentemente utilizados nos sistemas de irrigação por gotejamento no Brasil. Para realização do estudo, foi tomada uma amostra de 25 gotejadores de cada modelo. Na avaliação dos respectivos tubos emissores, foram determinados os seguintes parâmetros: (a) vazão média, (b) coeficiente de variação de fabricação, (c) espessura da parede (d), equação característica do gotejador, (e) diâmetro interno do tubo, (f) espaçamento entre emissores, (g) resistência à pressão com água na temperatura ambiente e à temperatura de 40oC, e (h) resistência do tubo à tração com tensão de 160 N e 180 N. As análises mostraram coeficientes de variação de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avaliação; Emissor; Irrigação por gotejamento.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782015000801439