Consulta: creatorFacets:"Detcheverry, Sebastien"
Registros recuperados: 2
Data/hora: 10/06/2024 15:02:43

Monitoring of sea scallops Placopecten magellanicus in bottom seeding trials using video in Miquelon bay, Saint Pierre et Miquelon, France
Provedor de dados: 5
Autores: Robert, Stephane; Le Moine, Olivier; Lunven, Michel; Caisey, Xavier; Gaffet, Jean-dominique; Le Gall, Erwan; Vasquez, Mickael; Rodriguez, Julien; Detcheverry, Sebastien; Goulletquer, Philippe.
Placopecten magellanicus production in Saint Pierre et Miquelon (NW North Atlantic) has been developed through direct seeding of juveniles on leased areas. However, most of the culture occurs in deep water ranging from 30 to 70 meters, which requires a monitoring by video to facilitate the grow-out and survival evaluation. In August 2008, a submersible leaded structure was connected by a video cable to the surface and observation screen was defined through the video, an altimeter and two lasers. The pictures were recorded on board on hard drive and digital video recorder DVCAM, and data were georeferenced by VIDEONAV software. Analysing the video tapes allows to establish a thematic database on the ground structure, presence or absence of seeded and wild...
Tipo: Text
Palavras-chave: Scallops; Placopecten magellanicus; GIS; Monitoring; Miquelon Bay.
Ano: 2009
URL: http://archimer.ifremer.fr/doc/00134/24544/22576.pdf

Méthode de cartographie quantitative des fonds marins par vidéo. Application au suivi des semis de Placopecten magellinacus en Rade de Miquelon.
Provedor de dados: 5
Autores: Lunven, Michel; Robert, Stephane; Caisey, Xavier; Rodriguez, Julien; Detcheverry, Sebastien; Gaffet, Jean-dominique; Le Gall, Erwan; Vasquez, Mickael.
Ce poster présente une méthodologie d’investigation des fonds marin par vidéo sous marine. Le système est constitué d’un bâti intégrant une caméra, un projecteur, un altimètre ainsi que des pointeurs laser. Les images vidéo des fonds marins sont retransmises et enregistrées à bord du navire sur disque dur et magnétoscope numérique DVCAM.  Lors des profils vidéo, le logiciel de gestion VIDEONAV permet de constituer un fichier de navigation intégrant les positions géographiques, le code temps du magnétoscope ainsi que la surface visualisée calculée à partir de la hauteur de prise de vue par rapport au fond. En temps différé, VIDEONAV permet le rejeu de la navigation et des bandes vidéo associées dans le but de compléter ou de générer des fichiers de...
Tipo: Text
Ano: 2009
URL: http://archimer.ifremer.fr/doc/00144/25516/23656.pdf