Consulta: creatorFacets:"Jasper,Samir P."
Registros recuperados: 7
Data/hora: 16/06/2024 00:34:50

Semeadora-adubadora: mecanismos de corte de palha e cargas verticais aplicadas
Provedor de dados: 91
Autores: Silva,Paulo R. A.; Benez,Sérgio H.; Jasper,Samir P.; Seki,André S.; Masiero,Fabrício C.; Riquetti,Neilor B.
Realizou-se este trabalho com o objetivo de avaliar o desempenho dos mecanismos de corte de palha de uma semeadora-adubadora em diferentes coberturas vegetais e cargas verticais aplicadas. O delineamento experimental utilizado foi em blocos ao acaso e esquema fatorial 3 x 4, com 4 repetições. Os trabalhos foram realizados com três diferentes mecanismos de corte de palha (disco liso, disco corrugado e disco ondulado) utilizando-se quatro diferentes cargas verticais (750, 1500, 2250 e 3000 N) em cinco coberturas de palha (milho, sorgo, aveia preta, triticale e nabiça). Os resultados mostraram que quanto maior a quantidade de matéria seca da cobertura vegetal maior também é a demanda de forças horizontal e vertical. O disco de corte ondulado possibilita os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantio direto; Cultura de cobertura; Interação ferramenta-solo.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662012001200015

ENERGY PERFORMANCE IN DISC HARROWING OPERATION IN DIFFERENT GRADIENTS AND GAUGES
Provedor de dados: 70
Autores: Oiole,Yasser A.; Kmiecik,Leonardo L.; Parize,Guilherme L.; Silva,Thiago X. da; Jasper,Samir P.
ABSTRACT The operational performance of the agricultural tractor can be increased by adjusting parameters such as tire inflation pressure, axle mass distribution and gauge opening, which is a very divergent factor in controlled-traffic production. The objective of the experiment was to measure the energy performance of a 93 kW agricultural tractor in intermediate grading operation in two slopes (flat and sloping) and three gauge configurations (closed, intermediate and open) in mobilized soil. Energy performance was determined from the following parameters: slip, engine speed, actual effective speed, hourly and specific fuel consumption; strength, power and performance on the drawbar. Turbo pressure and temperature monitoring was also performed at six...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuel consumption; Operating yield; Controlled trafic.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600769

OPERATIONAL AND ENERGY PERFORMANCE OF 250 kW DOUBLE WHEELED VERSUS RUBBER HALF-TRACKED TRACTORS IN THE SOYBEAN SOWING
Provedor de dados: 70
Autores: Neto,Lauro S.; Kmiecik,Leonardo L.; Jasper,Samir P.; Zimmermann,Gabriel G.; Savi,Daniel.
ABSTRACT The technological innovation in agriculture seeks to improve the performance of mechanized assemblies and, currently, rubber half-tracks are a valuable solution for agricultural tractors, combining traction performance and less soil compaction. The objective of the experiment was to evaluate the operational and energy performance of double wheeled versus rubber half-tracked agricultural tractors in the soybean sowing. The experiment was conducted in a strip-plot design with a double factorial arrangement (2×3). The first factor consisted of a tractor with double wheels on the front and rear axles versus a tractor with single wheels on the front axle and rubber half-tracks on the rear axle, while the second factor consisted of three different...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Slippage; Operating speed; Hourly fuel consumption.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500617

INFLUENCE OF SEED TUBE CURVATURE ON SEED LONGITUDINAL DISTRIBUTION
Provedor de dados: 70
Autores: Savi,Daniel; Kmiecik,Leonardo L.; Strapasson Neto,Lauro; Silva,Thiago X. da; Jasper,Samir P.
ABSTRACT Studies on the longitudinal distribution of seeds in the sowing row seek to improve crop homogeneity, thus generating high productivity. In this context, seed tubes must be analyzed for their angular curvature. Thus, this study aimed to evaluate the influence of the seed tube curvature on the longitudinal distribution of corn and soybean seeds at different speeds. Two experiments were conducted completely randomized in a double factorial design. The first factor consisted of the seed tube curvature (straight and curved) and the second factor consisted of sowing speeds (1.11, 1.39, and 1.67 m s−1 for corn and 1.39, 1.67, 1.94, and 2.22 m s−1 for soybean), with five replications. The parameters analyzed to measure the longitudinal distribution were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sowing uniformity; Productivity; Seed drill; Performance monitoring; Bench experiment.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600732

INTERFERENCE OF THE NUMBER OF REMOTE CONTROL VALVES IN USE ON THE ENERGY PERFORMANCE OF AN AGRICULTURAL TRACTOR WITH PRODUCTIVITY MANAGEMENT
Provedor de dados: 70
Autores: Neto,Lauro S.; Kmiecik,Leonardo L.; Jasper,Samir P.; Zimmermann,Gabriel G.; Savi,Daniel.
ABSTRACT The hydraulic remote control system allows the transfer of energy from the engine through a flow of hydraulic oil to engines and implements pulled by agricultural tractors, which can interfere with its energy and operational performance. This study aimed to evaluate the interference of the number of remote control valves in use on the operational and energy performance of an agricultural tractor, using a productivity management system. The experiment was conducted in a strip-plot design, with five replications and three treatments, which consisted of the number of remote control valves in use (1, 2, or 3), totaling 15 experimental units. The results were subjected to normality and homogeneity tests and analysis of variance, followed by the Tukey...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Power on the drawbar; Hydraulic system; Operational speed; Specific consumption; Engine thermal efficiency.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300356

Viabilidade econômica de aquisição de um silo-secador para pequenas áreas de produção
Provedor de dados: 70
Autores: Jasper,Samir P.; Biaggioni,Marco A. M.; Ribeiro,Jader P.
O objetivo deste trabalho foi avaliar, por meio de simulação econômica, a viabilidade de aquisição de um silo-secador, para pequenas propriedades rurais, tendo como referências as opções de terceirizar o processo de secagem/armazenagem ou a comercialização do milho úmido. Em virtude da alta diversificação encontrada nas pequenas propriedades rurais, a simulação foi realizada considerando-se diferentes tamanhos de áreas exploradas com milho (10; 20; 30 e 40 ha), níveis de produtividade (3.900; 4.500 e 5.100 kg ha-1) e preços por saca de milho (R$ 13,03; R$ 19,69 e R$ 34,29), no Estado de São Paulo. Comparando as rentabilidades obtidas, notou-se a superioridade da receita líquida na aquisição do silo secador nas áreas de produção de 20 ha com produtividade...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Silo secador; Milho; Simulação econômica.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300017

Análise Energética da cultura do crambe (Crambe abyssinica hochst) produzida em plantio direto
Provedor de dados: 70
Autores: Jasper,Samir P.; Biaggioni,Marco A. M.; Silva,Paulo R. A.; Seki,André S.; Bueno,Osmar C.
O objetivo deste trabalho foi caracterizar o consumo de energia na implantação e condução da cultura do Crambe abyssinica Hochst, em sistema de plantio direto, na Fazenda Experimental Lageado, pertencente à Faculdade de Ciências Agronômicas - UNESP, localizada no município de Botucatu - SP. Avaliando a sustentabilidade do sistema, estimaram-se, a eficiência energética e a cultura do crambe. Para o levantamento dos componentes da estrutura de dispêndios, foram utilizados coeficientes energéticos preconizados em literaturas especializadas. As estruturas de dispêndios energéticos por tipo, fonte e forma demonstraram que a energia indireta participou com 65,03%; as fontes industrial, fóssil e biológica representaram 68,80%, 23,67% e 11,30%, respectivamente....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eficiência energética; Matérias-primas para biodiesel; Biocombustíveis.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300004